<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;LEDs&lt;/b&gt; Please read the Description in Devices and Packages&lt;p&gt;
http://www.lumileds.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;</description>
<packages>
<package name="LUXEON_REBEL">
<description>&lt;b&gt;LUXEON® Rebel LED&lt;/b&gt;&lt;p&gt;

Set DRC - Clearance - &lt;b&gt;Same Signals&lt;/b&gt; to &lt;b&gt;0&lt;/b&gt; to avoid DRC error message for Pad in SMD.&lt;br&gt;
Please read the Device's Description how to connect it correctly in the Schematic.&lt;p&gt;
Source: http://www.lumileds.com/pdfs/AB32.pdf&lt;br&gt;
http://www.lumileds.com/pdfs/DS56.pdf&lt;br&gt;
Footprint Rebel customer_070207.dxf</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUXEON_REBEL+COOLPAD">
<description>&lt;B&gt;LUXEON REBEL LED&lt;/b&gt; with cooling pads&lt;br&gt;
Please read also description in Layer 49 Reference.&lt;p&gt;
Stop and Cream Mask defined by &lt;b&gt;Footprint Rebel customer_070207.dxf&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LUXEON_THERMAL">
<pin name="TH" direction="pwr"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LUXEON_REBEL" prefix="LED">
<description>&lt;b&gt;LUXEON Rebel&lt;/b&gt;&lt;p&gt;

Display layer 93, Pins, and connect all contact points with a net.&lt;br&gt;
The thermal pads are defined in a separate gate with addlevel REQUEST.&lt;br&gt;
Draw a net named 'TH' and connect all thermal pads with it.&lt;br&gt;
Please read the Package's Description about DRC settings.&lt;p&gt;
Source: http://www.lumileds.com/pdfs/AB32.pdf</description>
<gates>
<gate name="A" symbol="LED"/>
<gate name="TH" symbol="LUXEON_THERMAL"/>
</gates>
<devices>
<device name="" package="LUXEON_REBEL">
<connects>
<connect gate="A" pin="A" pad="A A@1" route="any"/>
<connect gate="A" pin="C" pad="C C@1" route="any"/>
<connect gate="TH" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00&lt;br&gt;
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON_REBEL+COOLPAD" prefix="LED">
<description>&lt;B&gt;LUXEON REBEL LED&lt;/b&gt; with cooling pads&lt;br&gt;
Display Layer &lt;b&gt;Refence&lt;/b&gt; in Board for more information&lt;p&gt;
Stop and Cream Mask defined by &lt;b&gt;Luxeon Rebel Footprint _customer.dxf&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="TH" symbol="LUXEON_THERMAL"/>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LUXEON_REBEL+COOLPAD">
<connects>
<connect gate="G$1" pin="A" pad="A A@1" route="any"/>
<connect gate="G$1" pin="C" pad="C C@1" route="any"/>
<connect gate="TH" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4 TH@5 TH@6 TH@7 TH@8 TH@9 TH@10 TH@11 TH@12 TH@13 TH@14 TH@15 TH@16 TH@17 TH@18 TH@19 TH@20 TH@21 TH@22 TH@23 TH@24 TH@25 TH@26 TH@27 TH@28 TH@29 TH@30 TH@31 TH@32 TH@33 TH@34 TH@35" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
