<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;PCI 9056 Data Book, Version 0.91© 2001 PLX Technology, Inc.&lt;/b&gt;&lt;p&gt;
All rights reserved.&lt;br&gt;
CONFIDENTIAL &amp; PROPRIETARY PRELIMINARY&lt;br&gt;
870 Maude Avenue, Sunnyvale,&lt;br&gt;
CA USA 94085</description>
<packages>
<package name="PBGA256">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt; PBGA 256</description>
</package>
<package name="TQFP64">
<description>&lt;b&gt;64-PIN PLASTIC TQFP&lt;/b&gt; (10x10)&lt;p&gt;
shrink quad flat pack, square&lt;br&gt;
Source: SQFP-S-10X10-64 ipc-smd.lbr</description>
</package>
<package name="QFP18-176">
<description>&lt;b&gt;QFP18-176&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 10&lt;/i&gt;&lt;br&gt;
Source: http://www1.plxtech.com/TEMP/77131/9030db-14.pdf</description>
</package>
<package name="FBGA64">
<description>&lt;b&gt;64-Ball Plastic FBGA&lt;/b&gt; 6 x 6 mm&lt;p&gt;
Source: http://www1.plxtech.com/TEMP/77131/NET2272r1A_data_book_v1.92_31Oct05.pdf</description>
</package>
<package name="PBGA337">
<description>&lt;b&gt;PEX 8311 337-Ball PBGA Package&lt;/b&gt;&lt;p&gt;
Source: www.plxtech.com ... PEX_8311AA_Data_Book_v0.90_10Apr06.pdf</description>
</package>
</packages>
<symbols>
<symbol name="PCI9056">
<pin name="!IRDY"/>
<pin name="!LOCK"/>
<pin name="PLCK" direction="in"/>
<pin name="PAR"/>
<pin name="!FRAME"/>
<pin name="!STOP"/>
<pin name="!PERR"/>
<pin name="C/!BE1"/>
<pin name="C/!BE0"/>
<pin name="!GNT1" direction="out"/>
<pin name="!GNT0/!REQ" direction="out"/>
<pin name="IDSEL" direction="in"/>
<pin name="C/!BE2"/>
<pin name="!DEVSEL"/>
<pin name="!SERR"/>
<pin name="!REQ2" direction="in"/>
<pin name="!GNT2" direction="out"/>
<pin name="TDO"/>
<pin name="!INTA"/>
<pin name="C/!BE3"/>
<pin name="!TRDY"/>
<pin name="!REQ1" direction="in"/>
<pin name="!GNT4" direction="out"/>
<pin name="!REQ4" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="!RST"/>
<pin name="REQ0/!GNT" direction="in"/>
<pin name="!GNT3" direction="out"/>
<pin name="!REQ3" direction="in"/>
<pin name="!GNT5" direction="out"/>
<pin name="!GNT6" direction="out"/>
<pin name="!PME"/>
<pin name="!BD_SEL" direction="in"/>
<pin name="!TRSRT" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="!REQ5" direction="in"/>
<pin name="!ENUM" direction="out"/>
<pin name="!REQ6" direction="in"/>
<pin name="CPCISW" direction="in"/>
<pin name="!IDDQEN" direction="in"/>
<pin name="!PMEREQ" direction="in"/>
<pin name="!LEDON" direction="out"/>
<pin name="EECS" direction="out"/>
<pin name="EESK" direction="out"/>
<pin name="EEDI/EEDO"/>
<pin name="PRESENT_DET" direction="in"/>
<pin name="!CSS" direction="in"/>
<pin name="!DACK0" direction="out"/>
<pin name="!DREQ0" direction="in"/>
<pin name="!DACK1" direction="out"/>
<pin name="!DREQ1" direction="in"/>
<pin name="USERO/!LLOCKO"/>
<pin name="USERI/LLOCKI" direction="in"/>
<pin name="!LINTO" direction="out"/>
<pin name="!LINTI" direction="in"/>
<pin name="!LRESET"/>
<pin name="!MDREQ/!DMPAF/!EOT"/>
<pin name="!HOSTEN" direction="in"/>
<pin name="!BDIP/!WAIT"/>
<pin name="!TS/!ADS"/>
<pin name="!BB/BREQI" direction="in"/>
<pin name="!RETRY/BREQO" direction="out"/>
<pin name="!TEA/!LSERR"/>
<pin name="DP0/DP3"/>
<pin name="!BI/!MTREM" direction="in"/>
<pin name="!BURST/!BLAST"/>
<pin name="!BG/LHOLDA" direction="in"/>
<pin name="DP1/DP2"/>
<pin name="DP3/DP0"/>
<pin name="RD/!WR/LW/!R"/>
<pin name="MODE1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="!TA/!READY"/>
<pin name="TSIZ1/!LBE2"/>
<pin name="!BR/LHOLD" direction="out"/>
<pin name="DP2/DP1"/>
<pin name="LCLK" direction="in"/>
<pin name="TSIZ0/!LBE3"/>
<pin name="2.5VAUX" direction="pwr"/>
<pin name="CARD_VAUX" direction="pwr"/>
<pin name="!BIGEND/!WAIT1"/>
</symbol>
<symbol name="PCI-LA">
<pin name="LA0/LA31/DT/!R" direction="in"/>
<pin name="LA1/LA30/!DEN" direction="in"/>
<pin name="LA2/LA29/ALE" direction="in"/>
<pin name="LA3/LA28" direction="in"/>
<pin name="LA4/LA27" direction="in"/>
<pin name="LA5/LA26" direction="in"/>
<pin name="LA6/LA25" direction="in"/>
<pin name="LA9/LA22" direction="in"/>
<pin name="LA8/LA23" direction="in"/>
<pin name="LA7/LA24" direction="in"/>
<pin name="LA14/LA17" direction="in"/>
<pin name="LA12/LA19" direction="in"/>
<pin name="LA11/LA20" direction="in"/>
<pin name="LA10/LA21" direction="in"/>
<pin name="LA20/LA11" direction="in"/>
<pin name="LA15/LA16" direction="in"/>
<pin name="LA16/LA15" direction="in"/>
<pin name="LA13/LA18" direction="in"/>
<pin name="LA24/LA7" direction="in"/>
<pin name="LA21/LA10" direction="in"/>
<pin name="LA18/LA13" direction="in"/>
<pin name="LA17/LA14" direction="in"/>
<pin name="LA29/LA2" direction="in"/>
<pin name="LA25/LA6" direction="in"/>
<pin name="LA23/LA8" direction="in"/>
<pin name="LA19/LA12" direction="in"/>
<pin name="LA31/!LBE0" direction="in"/>
<pin name="LA27/LA4" direction="in"/>
<pin name="LA22/LA9" direction="in"/>
<pin name="LA28/LA3" direction="in"/>
<pin name="LA26/LA5" direction="in"/>
<pin name="LA30/!LBE1" direction="in"/>
</symbol>
<symbol name="PCI-LD">
<pin name="LD20/LD11/LAD11" direction="in"/>
<pin name="LD4/LD27/LAD27" direction="in"/>
<pin name="LD1/LD30/LAD30" direction="in"/>
<pin name="LD30/LD1/LAD1" direction="in"/>
<pin name="LD27/LD4/LAD4" direction="in"/>
<pin name="LD23/LD8/LAD8" direction="in"/>
<pin name="LD19/LD12/LAD12" direction="in"/>
<pin name="LD14/LD17/LAD17" direction="in"/>
<pin name="LD11/LD20/LAD20" direction="in"/>
<pin name="LD7/LD24/LAD24" direction="in"/>
<pin name="LD3/LD28/LAD28" direction="in"/>
<pin name="LD28/LD3/LAD3" direction="in"/>
<pin name="LD26/LD5/LAD5" direction="in"/>
<pin name="LD22/LD9/LAD9" direction="in"/>
<pin name="LD18/LD13/LAD13" direction="in"/>
<pin name="LD15/LD16/LAD16" direction="in"/>
<pin name="LD12/LD19/LAD19" direction="in"/>
<pin name="LD8LD23/LAD23" direction="in"/>
<pin name="LD6/LD25/LAD25" direction="in"/>
<pin name="LD2LD29/LAD29" direction="in"/>
<pin name="LD31/LD0/LAD0" direction="in"/>
<pin name="LD25/LD6/LAD6" direction="in"/>
<pin name="LD24/LD7/LAD7" direction="in"/>
<pin name="LD21/LD10/LAD10" direction="in"/>
<pin name="LD17/LD14/LAD14" direction="in"/>
<pin name="LD16/LD15/LAD15" direction="in"/>
<pin name="LD13/LD18/LAD18" direction="in"/>
<pin name="LD10/LD21/LAD21" direction="in"/>
<pin name="LD9/LD22/LAD22" direction="in"/>
<pin name="LD5/LD26/LAD26" direction="in"/>
<pin name="LD0/LD31/LAD31" direction="in"/>
<pin name="LD29/LD2/LAD2" direction="in"/>
</symbol>
<symbol name="PWR-PCI9056">
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VIO@1" direction="pwr"/>
<pin name="VIO@2" direction="pwr"/>
<pin name="VIO@3" direction="pwr"/>
<pin name="VIO@4" direction="pwr"/>
<pin name="VCORE@1" direction="pwr"/>
<pin name="VCORE@2" direction="pwr"/>
<pin name="VCORE@3" direction="pwr"/>
<pin name="VCORE@4" direction="pwr"/>
<pin name="VCORE@5" direction="pwr"/>
<pin name="VCORE@6" direction="pwr"/>
<pin name="VRING@1" direction="pwr"/>
<pin name="VRING@2" direction="pwr"/>
<pin name="VRING@3" direction="pwr"/>
<pin name="VRING@4" direction="pwr"/>
<pin name="VRING@5" direction="pwr"/>
<pin name="VRING@6" direction="pwr"/>
<pin name="VRING@7" direction="pwr"/>
<pin name="VRING@8" direction="pwr"/>
<pin name="VRING@9" direction="pwr"/>
<pin name="VRING@10" direction="pwr"/>
<pin name="VRING@11" direction="pwr"/>
<pin name="VRING@12" direction="pwr"/>
<pin name="VRING@13" direction="pwr"/>
</symbol>
<symbol name="PCI-AD">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
</symbol>
<symbol name="NET2272">
<pin name="VSSC@1" direction="pwr"/>
<pin name="VSSC@2" direction="pwr"/>
<pin name="VDDC@1" direction="pwr"/>
<pin name="VDDC@2" direction="pwr"/>
<pin name="VDDIO@1" direction="pwr"/>
<pin name="VDDIO@2" direction="pwr"/>
<pin name="VDDIO@3" direction="pwr"/>
<pin name="VSSIO@1" direction="pwr"/>
<pin name="VSSIO@2" direction="pwr"/>
<pin name="VSSIO@3" direction="pwr"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="RSDP" direction="out"/>
<pin name="RSDM" direction="out"/>
<pin name="RPU" direction="out"/>
<pin name="RREF" direction="in"/>
<pin name="VDD2.5@1" direction="pwr"/>
<pin name="VDD3.3@1" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AVSS@1" direction="pwr"/>
<pin name="AVSS@2" direction="pwr"/>
<pin name="COM_AVSS" direction="pwr"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="LCLKO" direction="out"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="VBUS" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TMC2" direction="in"/>
<pin name="LA0" direction="in"/>
<pin name="LA1" direction="in"/>
<pin name="LA2" direction="in"/>
<pin name="LA3" direction="in"/>
<pin name="LA4" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="LD0"/>
<pin name="LD1"/>
<pin name="LD2"/>
<pin name="LD3"/>
<pin name="LD4"/>
<pin name="LD5"/>
<pin name="LD6"/>
<pin name="LD7"/>
<pin name="LD8"/>
<pin name="LD9"/>
<pin name="LD10"/>
<pin name="LD11"/>
<pin name="LD12"/>
<pin name="LD13"/>
<pin name="LD14"/>
<pin name="LD15"/>
<pin name="!IOR" direction="in" function="dot"/>
<pin name="!IOW" direction="in" function="dot"/>
<pin name="!IRQ" direction="out" function="dot"/>
<pin name="!CS" direction="in" function="dot"/>
<pin name="!DMAWR" direction="in" function="dot"/>
<pin name="!DMARD" direction="in" function="dot"/>
<pin name="DREQ" direction="out"/>
<pin name="DACK" direction="in"/>
<pin name="EOT" direction="in"/>
</symbol>
<symbol name="PAX8311">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="ADS"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="BAR0ENB" direction="in"/>
<pin name="BD_SEL" direction="in"/>
<pin name="BIGEND" direction="in"/>
<pin name="BLAST"/>
<pin name="BREQI" direction="in"/>
<pin name="BREQO" direction="out"/>
<pin name="BTERM"/>
<pin name="BTON" direction="in"/>
<pin name="BUNRI" direction="in"/>
<pin name="C/BE0"/>
<pin name="C/BE1"/>
<pin name="C/BE2"/>
<pin name="C/BE3"/>
<pin name="CCS" direction="in"/>
<pin name="DACK0" direction="out"/>
<pin name="DACK1" direction="out"/>
<pin name="DEVSEL"/>
<pin name="DMPAF/EOT"/>
<pin name="DP0"/>
<pin name="DP1"/>
<pin name="DP2"/>
<pin name="DP3"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="EECLK" direction="out"/>
<pin name="EECS" direction="out"/>
<pin name="EECS_2"/>
<pin name="EEDI/EEDO"/>
<pin name="EERDDATA" direction="out"/>
<pin name="EESK" direction="out"/>
<pin name="EEWRDATA"/>
<pin name="PLXT2" direction="in"/>
<pin name="ROOT_COMPLEX" direction="in"/>
<pin name="FRAME"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@40" direction="pwr"/>
<pin name="GND@41" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="GND@49" direction="pwr"/>
<pin name="GND@50" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@54" direction="pwr"/>
<pin name="GND@55" direction="pwr"/>
<pin name="GND@56" direction="pwr"/>
<pin name="GND@57" direction="pwr"/>
<pin name="GND@58" direction="pwr"/>
<pin name="GND@59" direction="pwr"/>
<pin name="GND@60" direction="pwr"/>
<pin name="GND@61" direction="pwr"/>
<pin name="GND@62" direction="pwr"/>
<pin name="GND@63" direction="pwr"/>
<pin name="GND@64" direction="pwr"/>
<pin name="GND@65" direction="pwr"/>
<pin name="GND@66" direction="pwr"/>
<pin name="GND@67" direction="pwr"/>
<pin name="GND@68" direction="pwr"/>
<pin name="GND@69" direction="pwr"/>
<pin name="GND@70" direction="pwr"/>
<pin name="GND@71" direction="pwr"/>
<pin name="GND@72" direction="pwr"/>
<pin name="GND@73" direction="pwr"/>
<pin name="GND@74" direction="pwr"/>
<pin name="GND@75" direction="pwr"/>
<pin name="GND@76" direction="pwr"/>
<pin name="GND@77" direction="pwr"/>
<pin name="GND@78" direction="pwr"/>
<pin name="GND@79" direction="pwr"/>
<pin name="GND@80" direction="pwr"/>
<pin name="GND@81" direction="pwr"/>
<pin name="GND@82" direction="pwr"/>
<pin name="GND@83" direction="pwr"/>
<pin name="GND@84" direction="pwr"/>
<pin name="GND@85" direction="pwr"/>
<pin name="GNT0"/>
<pin name="GNT1"/>
<pin name="GNT2"/>
<pin name="GNT3"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="IDDQEN" direction="in"/>
<pin name="INTA"/>
<pin name="INTB"/>
<pin name="INTC"/>
<pin name="INTD"/>
<pin name="IRDY"/>
<pin name="LA2"/>
<pin name="LA3"/>
<pin name="LA4"/>
<pin name="LA5"/>
<pin name="LA6"/>
<pin name="LA7"/>
<pin name="LA8"/>
<pin name="LA9"/>
<pin name="LA10"/>
<pin name="LA11"/>
<pin name="LA12"/>
<pin name="LA13"/>
<pin name="LA14"/>
<pin name="LA15"/>
<pin name="LA16"/>
<pin name="LA17"/>
<pin name="LA18"/>
<pin name="LA19"/>
<pin name="LA20"/>
<pin name="LA21"/>
<pin name="LA22"/>
<pin name="LA23"/>
<pin name="LA24"/>
<pin name="LA25"/>
<pin name="LA26"/>
<pin name="LA27"/>
<pin name="LA28"/>
<pin name="LA29/ALE"/>
<pin name="LA30/DEN"/>
<pin name="LA31/DTR/!R"/>
<pin name="LBE0"/>
<pin name="LBE1"/>
<pin name="LBE2"/>
<pin name="LBE3"/>
<pin name="LCLK" direction="in"/>
<pin name="LD0"/>
<pin name="LD1"/>
<pin name="LD2"/>
<pin name="LD3"/>
<pin name="LD4"/>
<pin name="LD5"/>
<pin name="LD6"/>
<pin name="LD7"/>
<pin name="LD8"/>
<pin name="LD9"/>
<pin name="LD10"/>
<pin name="LD11"/>
<pin name="LD12"/>
<pin name="LD13"/>
<pin name="LD14"/>
<pin name="LD15"/>
<pin name="LD16"/>
<pin name="LD17"/>
<pin name="LD18"/>
<pin name="LD19"/>
<pin name="LD20"/>
<pin name="LD21"/>
<pin name="LD22"/>
<pin name="LD23"/>
<pin name="LD24"/>
<pin name="LD25"/>
<pin name="LD26"/>
<pin name="LD27"/>
<pin name="LD28"/>
<pin name="LD29"/>
<pin name="LD30"/>
<pin name="LD31"/>
<pin name="LHOLD" direction="out"/>
<pin name="LHOLDA" direction="in"/>
<pin name="LINTI" direction="in"/>
<pin name="LINTO" direction="out"/>
<pin name="LOCK"/>
<pin name="LRESET"/>
<pin name="LSERR" direction="out"/>
<pin name="LW/R"/>
<pin name="PLXT1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="PAR"/>
<pin name="PCLKO" direction="out"/>
<pin name="PCLK_IN" direction="in"/>
<pin name="PERN0" direction="in"/>
<pin name="PERP0" direction="in"/>
<pin name="PERR"/>
<pin name="PERST"/>
<pin name="PETN0" direction="out"/>
<pin name="PETP0" direction="out"/>
<pin name="PEX8111_IDSEL"/>
<pin name="PMEIN" direction="in"/>
<pin name="PMEOUT" direction="out"/>
<pin name="PWR_OK" direction="out"/>
<pin name="READY"/>
<pin name="REFCLK+" direction="in"/>
<pin name="REFCLK-" direction="in"/>
<pin name="REQ0"/>
<pin name="REQ1"/>
<pin name="REQ2"/>
<pin name="REQ3"/>
<pin name="RST"/>
<pin name="SERR"/>
<pin name="SMC" direction="in"/>
<pin name="STOP"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="ITDO"/>
<pin name="TDO" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="TMC1" direction="in"/>
<pin name="TMC2" direction="in"/>
<pin name="TMC" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRDY"/>
<pin name="TRST" direction="in"/>
<pin name="USERI/LLOCKI" direction="in"/>
<pin name="USERO/LLOCKO" direction="out"/>
<pin name="VDD1_5_1" direction="pwr"/>
<pin name="VDD1_5_4" direction="pwr"/>
<pin name="VDD1_5_5" direction="pwr"/>
<pin name="VDD1_5_7" direction="pwr"/>
<pin name="VDD1_5_8" direction="pwr"/>
<pin name="VDD1_5_236" direction="pwr"/>
<pin name="VDD1_5_236@1" direction="pwr"/>
<pin name="VDD1_5_236@2" direction="pwr"/>
<pin name="VDD2_5_1" direction="pwr"/>
<pin name="VDD2_5_2" direction="pwr"/>
<pin name="VDD2_5_3" direction="pwr"/>
<pin name="VDD2_5_3@1" direction="pwr"/>
<pin name="VDD2_5_4" direction="pwr"/>
<pin name="VDD2_5_56" direction="pwr"/>
<pin name="VDD2_5_56@1" direction="pwr"/>
<pin name="VDD3_3" direction="pwr"/>
<pin name="VDD3_3@1" direction="pwr"/>
<pin name="VDD3_3@2" direction="pwr"/>
<pin name="VDD3_3@3" direction="pwr"/>
<pin name="VDD3_3@4" direction="pwr"/>
<pin name="VDD3_3@5" direction="pwr"/>
<pin name="VDD3_3@6" direction="pwr"/>
<pin name="VDD3_3@7" direction="pwr"/>
<pin name="VDD3_3@8" direction="pwr"/>
<pin name="VDD3_3@9" direction="pwr"/>
<pin name="VDD3_3@10" direction="pwr"/>
<pin name="VDD3_3@11" direction="pwr"/>
<pin name="VDD3_3@12" direction="pwr"/>
<pin name="VDD3_3@13" direction="pwr"/>
<pin name="VDD3_3@14" direction="pwr"/>
<pin name="VDD3_3@15" direction="pwr"/>
<pin name="VDD3_3@16" direction="pwr"/>
<pin name="VDD3_3@17" direction="pwr"/>
<pin name="VDD3_3@18" direction="pwr"/>
<pin name="VDD3_3@19" direction="pwr"/>
<pin name="VDD3_3@20" direction="pwr"/>
<pin name="VDD3_3@21" direction="pwr"/>
<pin name="VDD3_3@22" direction="pwr"/>
<pin name="VDD3_3@23" direction="pwr"/>
<pin name="VDD3_3@24" direction="pwr"/>
<pin name="VDD3_3@25" direction="pwr"/>
<pin name="VDD_P" direction="pwr"/>
<pin name="VDD_R" direction="pwr"/>
<pin name="VDD_T" direction="pwr"/>
<pin name="VSS_C" direction="pwr"/>
<pin name="VSS_P0" direction="pwr"/>
<pin name="VSS_P1" direction="pwr"/>
<pin name="VSS_R" direction="pwr"/>
<pin name="VSS_RE" direction="pwr"/>
<pin name="VSS_T" direction="pwr"/>
<pin name="WAIT"/>
<pin name="WAKEIN" direction="in"/>
<pin name="WAKEOUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PCI9056" prefix="IC">
<description>&lt;b&gt;PCI 9056&lt;/b&gt; PCI Bus Mastering I/O Accelerator&lt;p&gt;
between a 32-bit, 66 MHz PCI Bus and 32-bit, 66 MHz processor Local Bus&lt;br&gt;
Data Book Version 0.91b February 2002&lt;br&gt;
Website: http://www.plxtech.com</description>
<gates>
<gate name="A" symbol="PCI9056"/>
<gate name="B" symbol="PCI-LA"/>
<gate name="C" symbol="PCI-LD"/>
<gate name="D" symbol="PCI-AD"/>
<gate name="P" symbol="PWR-PCI9056"/>
</gates>
<devices>
<device name="" package="PBGA256">
<connects>
<connect gate="A" pin="!BB/BREQI" pad="A13"/>
<connect gate="A" pin="!BDIP/!WAIT" pad="C12"/>
<connect gate="A" pin="!BD_SEL" pad="B6"/>
<connect gate="A" pin="!BG/LHOLDA" pad="B14"/>
<connect gate="A" pin="!BI/!MTREM" pad="E13"/>
<connect gate="A" pin="!BIGEND/!WAIT1" pad="A9"/>
<connect gate="A" pin="!BR/LHOLD" pad="A16"/>
<connect gate="A" pin="!BURST/!BLAST" pad="A14"/>
<connect gate="A" pin="!CSS" pad="B9"/>
<connect gate="A" pin="!DACK0" pad="C9"/>
<connect gate="A" pin="!DACK1" pad="B10"/>
<connect gate="A" pin="!DEVSEL" pad="H3"/>
<connect gate="A" pin="!DREQ0" pad="A10"/>
<connect gate="A" pin="!DREQ1" pad="C10"/>
<connect gate="A" pin="!ENUM" pad="P6"/>
<connect gate="A" pin="!FRAME" pad="G2"/>
<connect gate="A" pin="!GNT0/!REQ" pad="A3"/>
<connect gate="A" pin="!GNT1" pad="T2"/>
<connect gate="A" pin="!GNT2" pad="T3"/>
<connect gate="A" pin="!GNT3" pad="N5"/>
<connect gate="A" pin="!GNT4" pad="R4"/>
<connect gate="A" pin="!GNT5" pad="R5"/>
<connect gate="A" pin="!GNT6" pad="T5"/>
<connect gate="A" pin="!HOSTEN" pad="B12"/>
<connect gate="A" pin="!IDDQEN" pad="B7"/>
<connect gate="A" pin="!INTA" pad="B4"/>
<connect gate="A" pin="!IRDY" pad="G1"/>
<connect gate="A" pin="!LEDON" pad="N7"/>
<connect gate="A" pin="!LINTI" pad="C11"/>
<connect gate="A" pin="!LINTO" pad="B11"/>
<connect gate="A" pin="!LOCK" pad="H1"/>
<connect gate="A" pin="!LRESET" pad="D11"/>
<connect gate="A" pin="!MDREQ/!DMPAF/!EOT" pad="A12"/>
<connect gate="A" pin="!PERR" pad="J2"/>
<connect gate="A" pin="!PME" pad="A6"/>
<connect gate="A" pin="!PMEREQ" pad="C7"/>
<connect gate="A" pin="!REQ1" pad="P4"/>
<connect gate="A" pin="!REQ2" pad="R3"/>
<connect gate="A" pin="!REQ3" pad="P5"/>
<connect gate="A" pin="!REQ4" pad="T4"/>
<connect gate="A" pin="!REQ5" pad="N6"/>
<connect gate="A" pin="!REQ6" pad="R6"/>
<connect gate="A" pin="!RETRY/BREQO" pad="B13"/>
<connect gate="A" pin="!RST" pad="C5"/>
<connect gate="A" pin="!SERR" pad="J3"/>
<connect gate="A" pin="!STOP" pad="H2"/>
<connect gate="A" pin="!TA/!READY" pad="C15"/>
<connect gate="A" pin="!TEA/!LSERR" pad="C13"/>
<connect gate="A" pin="!TRDY" pad="H4"/>
<connect gate="A" pin="!TRSRT" pad="C6"/>
<connect gate="A" pin="!TS/!ADS" pad="D12"/>
<connect gate="A" pin="2.5VAUX" pad="D7"/>
<connect gate="A" pin="C/!BE0" pad="N2"/>
<connect gate="A" pin="C/!BE1" pad="K2"/>
<connect gate="A" pin="C/!BE2" pad="G3"/>
<connect gate="A" pin="C/!BE3" pad="E4"/>
<connect gate="A" pin="CARD_VAUX" pad="A7"/>
<connect gate="A" pin="CPCISW" pad="T6"/>
<connect gate="A" pin="DP0/DP3" pad="D13"/>
<connect gate="A" pin="DP1/DP2" pad="C14"/>
<connect gate="A" pin="DP2/DP1" pad="B16"/>
<connect gate="A" pin="DP3/DP0" pad="D14"/>
<connect gate="A" pin="EECS" pad="A8"/>
<connect gate="A" pin="EEDI/EEDO" pad="C8"/>
<connect gate="A" pin="EESK" pad="B8"/>
<connect gate="A" pin="IDSEL" pad="D3"/>
<connect gate="A" pin="LCLK" pad="D16"/>
<connect gate="A" pin="MODE0" pad="B15"/>
<connect gate="A" pin="MODE1" pad="A15"/>
<connect gate="A" pin="PAR" pad="K1"/>
<connect gate="A" pin="PLCK" pad="J1"/>
<connect gate="A" pin="PRESENT_DET" pad="D8"/>
<connect gate="A" pin="RD/!WR/LW/!R" pad="P14"/>
<connect gate="A" pin="REQ0/!GNT" pad="D5"/>
<connect gate="A" pin="TCK" pad="B5"/>
<connect gate="A" pin="TDI" pad="D6"/>
<connect gate="A" pin="TDO" pad="A4"/>
<connect gate="A" pin="TMS" pad="A5"/>
<connect gate="A" pin="TSIZ0/!LBE3" pad="T16"/>
<connect gate="A" pin="TSIZ1/!LBE2" pad="P15"/>
<connect gate="A" pin="USERI/LLOCKI" pad="A11"/>
<connect gate="A" pin="USERO/!LLOCKO" pad="D10"/>
<connect gate="B" pin="LA0/LA31/DT/!R" pad="P7"/>
<connect gate="B" pin="LA1/LA30/!DEN" pad="R7"/>
<connect gate="B" pin="LA10/LA21" pad="T10"/>
<connect gate="B" pin="LA11/LA20" pad="R10"/>
<connect gate="B" pin="LA12/LA19" pad="P10"/>
<connect gate="B" pin="LA13/LA18" pad="T11"/>
<connect gate="B" pin="LA14/LA17" pad="N10"/>
<connect gate="B" pin="LA15/LA16" pad="P11"/>
<connect gate="B" pin="LA16/LA15" pad="R11"/>
<connect gate="B" pin="LA17/LA14" pad="T12"/>
<connect gate="B" pin="LA18/LA13" pad="R12"/>
<connect gate="B" pin="LA19/LA12" pad="T13"/>
<connect gate="B" pin="LA2/LA29/ALE" pad="T7"/>
<connect gate="B" pin="LA20/LA11" pad="N11"/>
<connect gate="B" pin="LA21/LA10" pad="P12"/>
<connect gate="B" pin="LA22/LA9" pad="T14"/>
<connect gate="B" pin="LA23/LA8" pad="R13"/>
<connect gate="B" pin="LA24/LA7" pad="N12"/>
<connect gate="B" pin="LA25/LA6" pad="P13"/>
<connect gate="B" pin="LA26/LA5" pad="T15"/>
<connect gate="B" pin="LA27/LA4" pad="R14"/>
<connect gate="B" pin="LA28/LA3" pad="R15"/>
<connect gate="B" pin="LA29/LA2" pad="N13"/>
<connect gate="B" pin="LA3/LA28" pad="N8"/>
<connect gate="B" pin="LA30/!LBE1" pad="R16"/>
<connect gate="B" pin="LA31/!LBE0" pad="N14"/>
<connect gate="B" pin="LA4/LA27" pad="P8"/>
<connect gate="B" pin="LA5/LA26" pad="R8"/>
<connect gate="B" pin="LA6/LA25" pad="T8"/>
<connect gate="B" pin="LA7/LA24" pad="T9"/>
<connect gate="B" pin="LA8/LA23" pad="R9"/>
<connect gate="B" pin="LA9/LA22" pad="P9"/>
<connect gate="C" pin="LD0/LD31/LAD31" pad="P16"/>
<connect gate="C" pin="LD1/LD30/LAD30" pad="M13"/>
<connect gate="C" pin="LD10/LD21/LAD21" pad="L16"/>
<connect gate="C" pin="LD11/LD20/LAD20" pad="K14"/>
<connect gate="C" pin="LD12/LD19/LAD19" pad="K15"/>
<connect gate="C" pin="LD13/LD18/LAD18" pad="K16"/>
<connect gate="C" pin="LD14/LD17/LAD17" pad="J14"/>
<connect gate="C" pin="LD15/LD16/LAD16" pad="J15"/>
<connect gate="C" pin="LD16/LD15/LAD15" pad="J16"/>
<connect gate="C" pin="LD17/LD14/LAD14" pad="H16"/>
<connect gate="C" pin="LD18/LD13/LAD13" pad="H15"/>
<connect gate="C" pin="LD19/LD12/LAD12" pad="H14"/>
<connect gate="C" pin="LD20/LD11/LAD11" pad="H13"/>
<connect gate="C" pin="LD21/LD10/LAD10" pad="G16"/>
<connect gate="C" pin="LD22/LD9/LAD9" pad="G15"/>
<connect gate="C" pin="LD23/LD8/LAD8" pad="G14"/>
<connect gate="C" pin="LD24/LD7/LAD7" pad="F16"/>
<connect gate="C" pin="LD25/LD6/LAD6" pad="E16"/>
<connect gate="C" pin="LD26/LD5/LAD5" pad="F15"/>
<connect gate="C" pin="LD27/LD4/LAD4" pad="F14"/>
<connect gate="C" pin="LD28/LD3/LAD3" pad="E15"/>
<connect gate="C" pin="LD29/LD2/LAD2" pad="D15"/>
<connect gate="C" pin="LD2LD29/LAD29" pad="N15"/>
<connect gate="C" pin="LD3/LD28/LAD28" pad="M14"/>
<connect gate="C" pin="LD30/LD1/LAD1" pad="E14"/>
<connect gate="C" pin="LD31/LD0/LAD0" pad="C16"/>
<connect gate="C" pin="LD4/LD27/LAD27" pad="L13"/>
<connect gate="C" pin="LD5/LD26/LAD26" pad="N16"/>
<connect gate="C" pin="LD6/LD25/LAD25" pad="M15"/>
<connect gate="C" pin="LD7/LD24/LAD24" pad="L14"/>
<connect gate="C" pin="LD8LD23/LAD23" pad="L15"/>
<connect gate="C" pin="LD9/LD22/LAD22" pad="M16"/>
<connect gate="D" pin="AD0" pad="P3"/>
<connect gate="D" pin="AD1" pad="R2"/>
<connect gate="D" pin="AD10" pad="N1"/>
<connect gate="D" pin="AD11" pad="M1"/>
<connect gate="D" pin="AD12" pad="L3"/>
<connect gate="D" pin="AD13" pad="L2"/>
<connect gate="D" pin="AD14" pad="L1"/>
<connect gate="D" pin="AD15" pad="K3"/>
<connect gate="D" pin="AD16" pad="F1"/>
<connect gate="D" pin="AD17" pad="F2"/>
<connect gate="D" pin="AD18" pad="E1"/>
<connect gate="D" pin="AD19" pad="F3"/>
<connect gate="D" pin="AD2" pad="R1"/>
<connect gate="D" pin="AD20" pad="D1"/>
<connect gate="D" pin="AD21" pad="E3"/>
<connect gate="D" pin="AD22" pad="D2"/>
<connect gate="D" pin="AD23" pad="C1"/>
<connect gate="D" pin="AD24" pad="C2"/>
<connect gate="D" pin="AD25" pad="A1"/>
<connect gate="D" pin="AD26" pad="B1"/>
<connect gate="D" pin="AD27" pad="B2"/>
<connect gate="D" pin="AD28" pad="C3"/>
<connect gate="D" pin="AD29" pad="D4"/>
<connect gate="D" pin="AD3" pad="T1"/>
<connect gate="D" pin="AD30" pad="A2"/>
<connect gate="D" pin="AD31" pad="C4"/>
<connect gate="D" pin="AD4" pad="P2"/>
<connect gate="D" pin="AD5" pad="M4"/>
<connect gate="D" pin="AD6" pad="N3"/>
<connect gate="D" pin="AD7" pad="P1"/>
<connect gate="D" pin="AD8" pad="M3"/>
<connect gate="D" pin="AD9" pad="L4"/>
<connect gate="P" pin="VCORE@1" pad="F4"/>
<connect gate="P" pin="VCORE@2" pad="K4"/>
<connect gate="P" pin="VCORE@3" pad="D9"/>
<connect gate="P" pin="VCORE@4" pad="F13"/>
<connect gate="P" pin="VCORE@5" pad="K13"/>
<connect gate="P" pin="VCORE@6" pad="N9"/>
<connect gate="P" pin="VIO@1" pad="B3"/>
<connect gate="P" pin="VIO@2" pad="E2"/>
<connect gate="P" pin="VIO@3" pad="M2"/>
<connect gate="P" pin="VIO@4" pad="N4"/>
<connect gate="P" pin="VRING@1" pad="E7"/>
<connect gate="P" pin="VRING@10" pad="H12"/>
<connect gate="P" pin="VRING@11" pad="J12"/>
<connect gate="P" pin="VRING@12" pad="K12"/>
<connect gate="P" pin="VRING@13" pad="M10"/>
<connect gate="P" pin="VRING@2" pad="E8"/>
<connect gate="P" pin="VRING@3" pad="G5"/>
<connect gate="P" pin="VRING@4" pad="H5"/>
<connect gate="P" pin="VRING@5" pad="K5"/>
<connect gate="P" pin="VRING@6" pad="M7"/>
<connect gate="P" pin="VRING@7" pad="M8"/>
<connect gate="P" pin="VRING@8" pad="E10"/>
<connect gate="P" pin="VRING@9" pad="G12"/>
<connect gate="P" pin="VSS@1" pad="E5"/>
<connect gate="P" pin="VSS@10" pad="G8"/>
<connect gate="P" pin="VSS@11" pad="H6"/>
<connect gate="P" pin="VSS@12" pad="H7"/>
<connect gate="P" pin="VSS@13" pad="H8"/>
<connect gate="P" pin="VSS@14" pad="J4"/>
<connect gate="P" pin="VSS@15" pad="J5"/>
<connect gate="P" pin="VSS@16" pad="J6"/>
<connect gate="P" pin="VSS@17" pad="J7"/>
<connect gate="P" pin="VSS@18" pad="J8"/>
<connect gate="P" pin="VSS@19" pad="K6"/>
<connect gate="P" pin="VSS@2" pad="E6"/>
<connect gate="P" pin="VSS@20" pad="K7"/>
<connect gate="P" pin="VSS@21" pad="K8"/>
<connect gate="P" pin="VSS@22" pad="L5"/>
<connect gate="P" pin="VSS@23" pad="L6"/>
<connect gate="P" pin="VSS@24" pad="L7"/>
<connect gate="P" pin="VSS@25" pad="L8"/>
<connect gate="P" pin="VSS@26" pad="M5"/>
<connect gate="P" pin="VSS@27" pad="M6"/>
<connect gate="P" pin="VSS@28" pad="E9"/>
<connect gate="P" pin="VSS@29" pad="E11"/>
<connect gate="P" pin="VSS@3" pad="F5"/>
<connect gate="P" pin="VSS@30" pad="E12"/>
<connect gate="P" pin="VSS@31" pad="F9"/>
<connect gate="P" pin="VSS@32" pad="F10"/>
<connect gate="P" pin="VSS@33" pad="F11"/>
<connect gate="P" pin="VSS@34" pad="F12"/>
<connect gate="P" pin="VSS@35" pad="G9"/>
<connect gate="P" pin="VSS@36" pad="G10"/>
<connect gate="P" pin="VSS@37" pad="G11"/>
<connect gate="P" pin="VSS@38" pad="G13"/>
<connect gate="P" pin="VSS@39" pad="H9"/>
<connect gate="P" pin="VSS@4" pad="F6"/>
<connect gate="P" pin="VSS@40" pad="H10"/>
<connect gate="P" pin="VSS@41" pad="H11"/>
<connect gate="P" pin="VSS@42" pad="J9"/>
<connect gate="P" pin="VSS@43" pad="J10"/>
<connect gate="P" pin="VSS@44" pad="J11"/>
<connect gate="P" pin="VSS@45" pad="J13"/>
<connect gate="P" pin="VSS@46" pad="K9"/>
<connect gate="P" pin="VSS@47" pad="K10"/>
<connect gate="P" pin="VSS@48" pad="K11"/>
<connect gate="P" pin="VSS@49" pad="L9"/>
<connect gate="P" pin="VSS@5" pad="F7"/>
<connect gate="P" pin="VSS@50" pad="L10"/>
<connect gate="P" pin="VSS@51" pad="L11"/>
<connect gate="P" pin="VSS@52" pad="L12"/>
<connect gate="P" pin="VSS@53" pad="M9"/>
<connect gate="P" pin="VSS@54" pad="M11"/>
<connect gate="P" pin="VSS@55" pad="M12"/>
<connect gate="P" pin="VSS@6" pad="F8"/>
<connect gate="P" pin="VSS@7" pad="G4"/>
<connect gate="P" pin="VSS@8" pad="G6"/>
<connect gate="P" pin="VSS@9" pad="G7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1623124"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NET2272" prefix="IC">
<description>&lt;b&gt;NET2272 USB 2.0 Peripheral Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.plxtech.com/dts/download.asp?f=NET2000/2272/Net2272.spec.re040615.pdf&lt;br&gt;
FBGA-Type: http://www1.plxtech.com/TEMP/77131/NET2272r1A_data_book_v1.92_31Oct05.pdf</description>
<gates>
<gate name="G$1" symbol="NET2272"/>
</gates>
<devices>
<device name="REV1A-LF" package="TQFP64">
<connects>
<connect gate="G$1" pin="!CS" pad="61"/>
<connect gate="G$1" pin="!DMARD" pad="50"/>
<connect gate="G$1" pin="!DMAWR" pad="34"/>
<connect gate="G$1" pin="!IOR" pad="59"/>
<connect gate="G$1" pin="!IOW" pad="60"/>
<connect gate="G$1" pin="!IRQ" pad="63"/>
<connect gate="G$1" pin="!RESET" pad="58"/>
<connect gate="G$1" pin="ALE" pad="53"/>
<connect gate="G$1" pin="AVDD" pad="15"/>
<connect gate="G$1" pin="AVSS@1" pad="12"/>
<connect gate="G$1" pin="AVSS@2" pad="14"/>
<connect gate="G$1" pin="COM_AVSS" pad="16"/>
<connect gate="G$1" pin="DACK" pad="51"/>
<connect gate="G$1" pin="DM" pad="8"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="DREQ" pad="62"/>
<connect gate="G$1" pin="EOT" pad="52"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="10"/>
<connect gate="G$1" pin="LA0" pad="32"/>
<connect gate="G$1" pin="LA1" pad="31"/>
<connect gate="G$1" pin="LA2" pad="30"/>
<connect gate="G$1" pin="LA3" pad="29"/>
<connect gate="G$1" pin="LA4" pad="28"/>
<connect gate="G$1" pin="LCLKO" pad="57"/>
<connect gate="G$1" pin="LD0" pad="19"/>
<connect gate="G$1" pin="LD1" pad="20"/>
<connect gate="G$1" pin="LD10" pad="43"/>
<connect gate="G$1" pin="LD11" pad="44"/>
<connect gate="G$1" pin="LD12" pad="45"/>
<connect gate="G$1" pin="LD13" pad="46"/>
<connect gate="G$1" pin="LD14" pad="47"/>
<connect gate="G$1" pin="LD15" pad="49"/>
<connect gate="G$1" pin="LD2" pad="21"/>
<connect gate="G$1" pin="LD3" pad="22"/>
<connect gate="G$1" pin="LD4" pad="23"/>
<connect gate="G$1" pin="LD5" pad="35"/>
<connect gate="G$1" pin="LD6" pad="36"/>
<connect gate="G$1" pin="LD7" pad="37"/>
<connect gate="G$1" pin="LD8" pad="38"/>
<connect gate="G$1" pin="LD9" pad="39"/>
<connect gate="G$1" pin="PVDD" pad="11"/>
<connect gate="G$1" pin="RPU" pad="2"/>
<connect gate="G$1" pin="RREF" pad="13"/>
<connect gate="G$1" pin="RSDM" pad="9"/>
<connect gate="G$1" pin="RSDP" pad="5"/>
<connect gate="G$1" pin="TEST" pad="18"/>
<connect gate="G$1" pin="TMC2" pad="17"/>
<connect gate="G$1" pin="TRST" pad="40"/>
<connect gate="G$1" pin="VBUS" pad="64"/>
<connect gate="G$1" pin="VDD2.5@1" pad="3"/>
<connect gate="G$1" pin="VDD3.3@1" pad="7"/>
<connect gate="G$1" pin="VDDC@1" pad="1"/>
<connect gate="G$1" pin="VDDC@2" pad="48"/>
<connect gate="G$1" pin="VDDIO@1" pad="27"/>
<connect gate="G$1" pin="VDDIO@2" pad="42"/>
<connect gate="G$1" pin="VDDIO@3" pad="55"/>
<connect gate="G$1" pin="VSSC@1" pad="24"/>
<connect gate="G$1" pin="VSSC@2" pad="56"/>
<connect gate="G$1" pin="VSSIO@1" pad="33"/>
<connect gate="G$1" pin="VSSIO@2" pad="41"/>
<connect gate="G$1" pin="VSSIO@3" pad="54"/>
<connect gate="G$1" pin="XIN" pad="25"/>
<connect gate="G$1" pin="XOUT" pad="26"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NET2272REV1A-LF"/>
<attribute name="OC_FARNELL" value="1623121"/>
<attribute name="OC_NEWARK" value="08P1483"/>
</technology>
</technologies>
</device>
<device name="REV1A-BCF" package="FBGA64">
<connects>
<connect gate="G$1" pin="!CS" pad="C7"/>
<connect gate="G$1" pin="!DMARD" pad="G7"/>
<connect gate="G$1" pin="!DMAWR" pad="H3"/>
<connect gate="G$1" pin="!IOR" pad="C8"/>
<connect gate="G$1" pin="!IOW" pad="B7"/>
<connect gate="G$1" pin="!IRQ" pad="D6"/>
<connect gate="G$1" pin="!RESET" pad="C6"/>
<connect gate="G$1" pin="ALE" pad="E8"/>
<connect gate="G$1" pin="AVDD" pad="C3"/>
<connect gate="G$1" pin="AVSS@1" pad="B2"/>
<connect gate="G$1" pin="AVSS@2" pad="B6"/>
<connect gate="G$1" pin="COM_AVSS" pad="A2"/>
<connect gate="G$1" pin="DACK" pad="F7"/>
<connect gate="G$1" pin="DM" pad="B3"/>
<connect gate="G$1" pin="DP" pad="B5"/>
<connect gate="G$1" pin="DREQ" pad="A8"/>
<connect gate="G$1" pin="EOT" pad="E7"/>
<connect gate="G$1" pin="GND@1" pad="A4"/>
<connect gate="G$1" pin="GND@2" pad="A6"/>
<connect gate="G$1" pin="LA0" pad="G1"/>
<connect gate="G$1" pin="LA1" pad="G2"/>
<connect gate="G$1" pin="LA2" pad="F2"/>
<connect gate="G$1" pin="LA3" pad="E2"/>
<connect gate="G$1" pin="LA4" pad="F1"/>
<connect gate="G$1" pin="LCLKO" pad="E6"/>
<connect gate="G$1" pin="LD0" pad="A1"/>
<connect gate="G$1" pin="LD1" pad="B1"/>
<connect gate="G$1" pin="LD10" pad="G6"/>
<connect gate="G$1" pin="LD11" pad="H5"/>
<connect gate="G$1" pin="LD12" pad="F6"/>
<connect gate="G$1" pin="LD13" pad="H6"/>
<connect gate="G$1" pin="LD14" pad="H7"/>
<connect gate="G$1" pin="LD15" pad="G8"/>
<connect gate="G$1" pin="LD2" pad="C2"/>
<connect gate="G$1" pin="LD3" pad="C1"/>
<connect gate="G$1" pin="LD4" pad="D3"/>
<connect gate="G$1" pin="LD5" pad="H2"/>
<connect gate="G$1" pin="LD6" pad="G3"/>
<connect gate="G$1" pin="LD7" pad="F3"/>
<connect gate="G$1" pin="LD8" pad="G4"/>
<connect gate="G$1" pin="LD9" pad="F4"/>
<connect gate="G$1" pin="PVDD" pad="C4"/>
<connect gate="G$1" pin="RPU" pad="D5"/>
<connect gate="G$1" pin="RREF" pad="D4"/>
<connect gate="G$1" pin="RSDM" pad="A3"/>
<connect gate="G$1" pin="RSDP" pad="A5"/>
<connect gate="G$1" pin="TEST" pad="E4"/>
<connect gate="G$1" pin="TMC2" pad="E5"/>
<connect gate="G$1" pin="TRST" pad="G5"/>
<connect gate="G$1" pin="VBUS" pad="B8"/>
<connect gate="G$1" pin="VDD2.5@1" pad="C5"/>
<connect gate="G$1" pin="VDD3.3@1" pad="B4"/>
<connect gate="G$1" pin="VDDC@1" pad="A7"/>
<connect gate="G$1" pin="VDDC@2" pad="H8"/>
<connect gate="G$1" pin="VDDIO@1" pad="D7"/>
<connect gate="G$1" pin="VDDIO@2" pad="E3"/>
<connect gate="G$1" pin="VDDIO@3" pad="F5"/>
<connect gate="G$1" pin="VSSC@1" pad="D2"/>
<connect gate="G$1" pin="VSSC@2" pad="D8"/>
<connect gate="G$1" pin="VSSIO@1" pad="F8"/>
<connect gate="G$1" pin="VSSIO@2" pad="H1"/>
<connect gate="G$1" pin="VSSIO@3" pad="H4"/>
<connect gate="G$1" pin="XIN" pad="E1"/>
<connect gate="G$1" pin="XOUT" pad="D1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PEX78311" prefix="IC">
<description>&lt;b&gt;PCI Express Endpoint Interface&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 16&lt;/i&gt; from &lt;b&gt;PEX8311_BSDL_netlist_r1.0.dat&lt;/b&gt;&lt;br&gt;
and manuell corrected&lt;br&gt;
Source: PEX_8311AA_Data_Book_v0.90_10Apr06.pdf</description>
<gates>
<gate name="G$1" symbol="PAX8311"/>
</gates>
<devices>
<device name="" package="PBGA337">
<connects>
<connect gate="G$1" pin="AD0" pad="T1"/>
<connect gate="G$1" pin="AD1" pad="P1"/>
<connect gate="G$1" pin="AD10" pad="R2"/>
<connect gate="G$1" pin="AD11" pad="N3"/>
<connect gate="G$1" pin="AD12" pad="M2"/>
<connect gate="G$1" pin="AD13" pad="P3"/>
<connect gate="G$1" pin="AD14" pad="V8"/>
<connect gate="G$1" pin="AD15" pad="N2"/>
<connect gate="G$1" pin="AD16" pad="T2"/>
<connect gate="G$1" pin="AD17" pad="P2"/>
<connect gate="G$1" pin="AD18" pad="N4"/>
<connect gate="G$1" pin="AD19" pad="V7"/>
<connect gate="G$1" pin="AD2" pad="W6"/>
<connect gate="G$1" pin="AD20" pad="R1"/>
<connect gate="G$1" pin="AD21" pad="U2"/>
<connect gate="G$1" pin="AD22" pad="Y6"/>
<connect gate="G$1" pin="AD23" pad="E6"/>
<connect gate="G$1" pin="AD24" pad="D4"/>
<connect gate="G$1" pin="AD25" pad="C5"/>
<connect gate="G$1" pin="AD26" pad="U4"/>
<connect gate="G$1" pin="AD27" pad="R3"/>
<connect gate="G$1" pin="AD28" pad="C10"/>
<connect gate="G$1" pin="AD29" pad="D11"/>
<connect gate="G$1" pin="AD3" pad="B12"/>
<connect gate="G$1" pin="AD30" pad="D5"/>
<connect gate="G$1" pin="AD31" pad="E4"/>
<connect gate="G$1" pin="AD4" pad="B11"/>
<connect gate="G$1" pin="AD5" pad="C11"/>
<connect gate="G$1" pin="AD6" pad="B13"/>
<connect gate="G$1" pin="AD7" pad="C8"/>
<connect gate="G$1" pin="AD8" pad="B7"/>
<connect gate="G$1" pin="AD9" pad="B9"/>
<connect gate="G$1" pin="ADS" pad="F19"/>
<connect gate="G$1" pin="AVDD" pad="G3"/>
<connect gate="G$1" pin="AVSS" pad="J3"/>
<connect gate="G$1" pin="BAR0ENB" pad="E1"/>
<connect gate="G$1" pin="BD_SEL" pad="B19"/>
<connect gate="G$1" pin="BIGEND" pad="D18"/>
<connect gate="G$1" pin="BLAST" pad="F20"/>
<connect gate="G$1" pin="BREQI" pad="G18"/>
<connect gate="G$1" pin="BREQO" pad="G17"/>
<connect gate="G$1" pin="BTERM" pad="J19"/>
<connect gate="G$1" pin="BTON" pad="D10"/>
<connect gate="G$1" pin="BUNRI" pad="F3"/>
<connect gate="G$1" pin="C/BE0" pad="W7"/>
<connect gate="G$1" pin="C/BE1" pad="U7"/>
<connect gate="G$1" pin="C/BE2" pad="C4"/>
<connect gate="G$1" pin="C/BE3" pad="C12"/>
<connect gate="G$1" pin="CCS" pad="D17"/>
<connect gate="G$1" pin="DACK0" pad="C20"/>
<connect gate="G$1" pin="DACK1" pad="B18"/>
<connect gate="G$1" pin="DEVSEL" pad="T3"/>
<connect gate="G$1" pin="DMPAF/EOT" pad="C18"/>
<connect gate="G$1" pin="DP0" pad="L16"/>
<connect gate="G$1" pin="DP1" pad="L15"/>
<connect gate="G$1" pin="DP2" pad="M16"/>
<connect gate="G$1" pin="DP3" pad="M15"/>
<connect gate="G$1" pin="DREQ0" pad="C19"/>
<connect gate="G$1" pin="DREQ1" pad="B17"/>
<connect gate="G$1" pin="EECLK" pad="L4"/>
<connect gate="G$1" pin="EECS" pad="A20"/>
<connect gate="G$1" pin="EECS_2" pad="K3"/>
<connect gate="G$1" pin="EEDI/EEDO" pad="B20"/>
<connect gate="G$1" pin="EERDDATA" pad="M3"/>
<connect gate="G$1" pin="EESK" pad="A19"/>
<connect gate="G$1" pin="EEWRDATA" pad="L3"/>
<connect gate="G$1" pin="FRAME" pad="P4"/>
<connect gate="G$1" pin="GND" pad="A2"/>
<connect gate="G$1" pin="GND@1" pad="A16"/>
<connect gate="G$1" pin="GND@10" pad="E8"/>
<connect gate="G$1" pin="GND@11" pad="E10"/>
<connect gate="G$1" pin="GND@12" pad="E11"/>
<connect gate="G$1" pin="GND@13" pad="E12"/>
<connect gate="G$1" pin="GND@14" pad="E13"/>
<connect gate="G$1" pin="GND@15" pad="E14"/>
<connect gate="G$1" pin="GND@16" pad="F6"/>
<connect gate="G$1" pin="GND@17" pad="F7"/>
<connect gate="G$1" pin="GND@18" pad="F8"/>
<connect gate="G$1" pin="GND@19" pad="F9"/>
<connect gate="G$1" pin="GND@2" pad="A17"/>
<connect gate="G$1" pin="GND@20" pad="F10"/>
<connect gate="G$1" pin="GND@21" pad="F11"/>
<connect gate="G$1" pin="GND@22" pad="F12"/>
<connect gate="G$1" pin="GND@23" pad="F13"/>
<connect gate="G$1" pin="GND@24" pad="F14"/>
<connect gate="G$1" pin="GND@25" pad="G5"/>
<connect gate="G$1" pin="GND@26" pad="G6"/>
<connect gate="G$1" pin="GND@27" pad="G7"/>
<connect gate="G$1" pin="GND@28" pad="H5"/>
<connect gate="G$1" pin="GND@29" pad="H6"/>
<connect gate="G$1" pin="GND@3" pad="B15"/>
<connect gate="G$1" pin="GND@30" pad="H15"/>
<connect gate="G$1" pin="GND@31" pad="J5"/>
<connect gate="G$1" pin="GND@32" pad="J6"/>
<connect gate="G$1" pin="GND@33" pad="J15"/>
<connect gate="G$1" pin="GND@34" pad="K4"/>
<connect gate="G$1" pin="GND@35" pad="K5"/>
<connect gate="G$1" pin="GND@36" pad="K6"/>
<connect gate="G$1" pin="GND@37" pad="K15"/>
<connect gate="G$1" pin="GND@38" pad="L5"/>
<connect gate="G$1" pin="GND@39" pad="L6"/>
<connect gate="G$1" pin="GND@4" pad="B16"/>
<connect gate="G$1" pin="GND@40" pad="M4"/>
<connect gate="G$1" pin="GND@41" pad="M5"/>
<connect gate="G$1" pin="GND@42" pad="M6"/>
<connect gate="G$1" pin="GND@43" pad="N5"/>
<connect gate="G$1" pin="GND@44" pad="N6"/>
<connect gate="G$1" pin="GND@45" pad="N15"/>
<connect gate="G$1" pin="GND@46" pad="P5"/>
<connect gate="G$1" pin="GND@47" pad="P6"/>
<connect gate="G$1" pin="GND@48" pad="P15"/>
<connect gate="G$1" pin="GND@49" pad="R5"/>
<connect gate="G$1" pin="GND@5" pad="D12"/>
<connect gate="G$1" pin="GND@50" pad="R6"/>
<connect gate="G$1" pin="GND@51" pad="R7"/>
<connect gate="G$1" pin="GND@52" pad="R8"/>
<connect gate="G$1" pin="GND@53" pad="R9"/>
<connect gate="G$1" pin="GND@54" pad="R10"/>
<connect gate="G$1" pin="GND@55" pad="R11"/>
<connect gate="G$1" pin="GND@56" pad="R12"/>
<connect gate="G$1" pin="GND@57" pad="R13"/>
<connect gate="G$1" pin="GND@58" pad="R14"/>
<connect gate="G$1" pin="GND@59" pad="R15"/>
<connect gate="G$1" pin="GND@6" pad="D13"/>
<connect gate="G$1" pin="GND@60" pad="T5"/>
<connect gate="G$1" pin="GND@61" pad="T6"/>
<connect gate="G$1" pin="GND@62" pad="T7"/>
<connect gate="G$1" pin="GND@63" pad="T8"/>
<connect gate="G$1" pin="GND@64" pad="T9"/>
<connect gate="G$1" pin="GND@65" pad="T10"/>
<connect gate="G$1" pin="GND@66" pad="T11"/>
<connect gate="G$1" pin="GND@67" pad="T13"/>
<connect gate="G$1" pin="GND@68" pad="T14"/>
<connect gate="G$1" pin="GND@69" pad="U5"/>
<connect gate="G$1" pin="GND@7" pad="D14"/>
<connect gate="G$1" pin="GND@70" pad="U6"/>
<connect gate="G$1" pin="GND@71" pad="U8"/>
<connect gate="G$1" pin="GND@72" pad="U9"/>
<connect gate="G$1" pin="GND@73" pad="U12"/>
<connect gate="G$1" pin="GND@74" pad="U13"/>
<connect gate="G$1" pin="GND@75" pad="V1"/>
<connect gate="G$1" pin="GND@76" pad="V12"/>
<connect gate="G$1" pin="GND@77" pad="V13"/>
<connect gate="G$1" pin="GND@78" pad="W1"/>
<connect gate="G$1" pin="GND@79" pad="W2"/>
<connect gate="G$1" pin="GND@8" pad="D15"/>
<connect gate="G$1" pin="GND@80" pad="W3"/>
<connect gate="G$1" pin="GND@81" pad="W4"/>
<connect gate="G$1" pin="GND@82" pad="Y1"/>
<connect gate="G$1" pin="GND@83" pad="Y2"/>
<connect gate="G$1" pin="GND@84" pad="Y3"/>
<connect gate="G$1" pin="GND@85" pad="Y4"/>
<connect gate="G$1" pin="GND@9" pad="E7"/>
<connect gate="G$1" pin="GNT0" pad="D16"/>
<connect gate="G$1" pin="GNT1" pad="B8"/>
<connect gate="G$1" pin="GNT2" pad="B5"/>
<connect gate="G$1" pin="GNT3" pad="B3"/>
<connect gate="G$1" pin="GPIO0" pad="C1"/>
<connect gate="G$1" pin="GPIO1" pad="B1"/>
<connect gate="G$1" pin="GPIO2" pad="D3"/>
<connect gate="G$1" pin="GPIO3" pad="A1"/>
<connect gate="G$1" pin="IDDQEN" pad="V10"/>
<connect gate="G$1" pin="INTA" pad="A5"/>
<connect gate="G$1" pin="INTB" pad="A6"/>
<connect gate="G$1" pin="INTC" pad="B4"/>
<connect gate="G$1" pin="INTD" pad="A4"/>
<connect gate="G$1" pin="IRDY" pad="U1"/>
<connect gate="G$1" pin="ITDO" pad="C15"/>
<connect gate="G$1" pin="LA10" pad="W16"/>
<connect gate="G$1" pin="LA11" pad="V16"/>
<connect gate="G$1" pin="LA12" pad="U16"/>
<connect gate="G$1" pin="LA13" pad="Y15"/>
<connect gate="G$1" pin="LA14" pad="W15"/>
<connect gate="G$1" pin="LA15" pad="V15"/>
<connect gate="G$1" pin="LA16" pad="Y14"/>
<connect gate="G$1" pin="LA17" pad="W14"/>
<connect gate="G$1" pin="LA18" pad="Y13"/>
<connect gate="G$1" pin="LA19" pad="W13"/>
<connect gate="G$1" pin="LA2" pad="Y18"/>
<connect gate="G$1" pin="LA20" pad="Y12"/>
<connect gate="G$1" pin="LA21" pad="W12"/>
<connect gate="G$1" pin="LA22" pad="Y11"/>
<connect gate="G$1" pin="LA23" pad="W11"/>
<connect gate="G$1" pin="LA24" pad="V11"/>
<connect gate="G$1" pin="LA25" pad="Y10"/>
<connect gate="G$1" pin="LA26" pad="W10"/>
<connect gate="G$1" pin="LA27" pad="Y9"/>
<connect gate="G$1" pin="LA28" pad="W9"/>
<connect gate="G$1" pin="LA29/ALE" pad="Y8"/>
<connect gate="G$1" pin="LA3" pad="W18"/>
<connect gate="G$1" pin="LA30/DEN" pad="W8"/>
<connect gate="G$1" pin="LA31/DTR/!R" pad="Y7"/>
<connect gate="G$1" pin="LA4" pad="V18"/>
<connect gate="G$1" pin="LA5" pad="Y17"/>
<connect gate="G$1" pin="LA6" pad="W17"/>
<connect gate="G$1" pin="LA7" pad="V17"/>
<connect gate="G$1" pin="LA8" pad="U17"/>
<connect gate="G$1" pin="LA9" pad="Y16"/>
<connect gate="G$1" pin="LBE0" pad="W19"/>
<connect gate="G$1" pin="LBE1" pad="W20"/>
<connect gate="G$1" pin="LBE2" pad="Y20"/>
<connect gate="G$1" pin="LBE3" pad="Y19"/>
<connect gate="G$1" pin="LCLK" pad="J20"/>
<connect gate="G$1" pin="LD0" pad="K20"/>
<connect gate="G$1" pin="LD1" pad="K19"/>
<connect gate="G$1" pin="LD10" pad="M18"/>
<connect gate="G$1" pin="LD11" pad="M17"/>
<connect gate="G$1" pin="LD12" pad="N20"/>
<connect gate="G$1" pin="LD13" pad="N19"/>
<connect gate="G$1" pin="LD14" pad="N18"/>
<connect gate="G$1" pin="LD15" pad="N17"/>
<connect gate="G$1" pin="LD16" pad="P20"/>
<connect gate="G$1" pin="LD17" pad="P19"/>
<connect gate="G$1" pin="LD18" pad="P18"/>
<connect gate="G$1" pin="LD19" pad="P17"/>
<connect gate="G$1" pin="LD2" pad="K18"/>
<connect gate="G$1" pin="LD20" pad="R20"/>
<connect gate="G$1" pin="LD21" pad="R19"/>
<connect gate="G$1" pin="LD22" pad="R18"/>
<connect gate="G$1" pin="LD23" pad="R17"/>
<connect gate="G$1" pin="LD24" pad="T20"/>
<connect gate="G$1" pin="LD25" pad="T19"/>
<connect gate="G$1" pin="LD26" pad="T18"/>
<connect gate="G$1" pin="LD27" pad="T17"/>
<connect gate="G$1" pin="LD28" pad="U20"/>
<connect gate="G$1" pin="LD29" pad="U19"/>
<connect gate="G$1" pin="LD3" pad="K17"/>
<connect gate="G$1" pin="LD30" pad="V20"/>
<connect gate="G$1" pin="LD31" pad="V19"/>
<connect gate="G$1" pin="LD4" pad="L20"/>
<connect gate="G$1" pin="LD5" pad="L19"/>
<connect gate="G$1" pin="LD6" pad="L18"/>
<connect gate="G$1" pin="LD7" pad="L17"/>
<connect gate="G$1" pin="LD8" pad="M20"/>
<connect gate="G$1" pin="LD9" pad="M19"/>
<connect gate="G$1" pin="LHOLD" pad="G20"/>
<connect gate="G$1" pin="LHOLDA" pad="G19"/>
<connect gate="G$1" pin="LINTI" pad="E20"/>
<connect gate="G$1" pin="LINTO" pad="E19"/>
<connect gate="G$1" pin="LOCK" pad="R4"/>
<connect gate="G$1" pin="LRESET" pad="E18"/>
<connect gate="G$1" pin="LSERR" pad="J18"/>
<connect gate="G$1" pin="LW/R" pad="U18"/>
<connect gate="G$1" pin="MODE0" pad="H19"/>
<connect gate="G$1" pin="MODE1" pad="H20"/>
<connect gate="G$1" pin="PAR" pad="V6"/>
<connect gate="G$1" pin="PCLKO" pad="A8"/>
<connect gate="G$1" pin="PCLK_IN" pad="A15"/>
<connect gate="G$1" pin="PERN0" pad="F2"/>
<connect gate="G$1" pin="PERP0" pad="G1"/>
<connect gate="G$1" pin="PERR" pad="T4"/>
<connect gate="G$1" pin="PERST" pad="C3"/>
<connect gate="G$1" pin="PETN0" pad="K2"/>
<connect gate="G$1" pin="PETP0" pad="J1"/>
<connect gate="G$1" pin="PEX8111_IDSEL" pad="A12"/>
<connect gate="G$1" pin="PLXT1" pad="A3"/>
<connect gate="G$1" pin="PLXT2" pad="A10"/>
<connect gate="G$1" pin="PMEIN" pad="C16"/>
<connect gate="G$1" pin="PMEOUT" pad="B10"/>
<connect gate="G$1" pin="PWR_OK" pad="D2"/>
<connect gate="G$1" pin="READY" pad="F18"/>
<connect gate="G$1" pin="REFCLK+" pad="H1"/>
<connect gate="G$1" pin="REFCLK-" pad="H2"/>
<connect gate="G$1" pin="REQ0" pad="C7"/>
<connect gate="G$1" pin="REQ1" pad="A9"/>
<connect gate="G$1" pin="REQ2" pad="A7"/>
<connect gate="G$1" pin="REQ3" pad="B6"/>
<connect gate="G$1" pin="ROOT_COMPLEX" pad="A18"/>
<connect gate="G$1" pin="RST" pad="C6"/>
<connect gate="G$1" pin="SERR" pad="U3"/>
<connect gate="G$1" pin="SMC" pad="V4"/>
<connect gate="G$1" pin="STOP" pad="V2"/>
<connect gate="G$1" pin="TCK" pad="A13"/>
<connect gate="G$1" pin="TDI" pad="A14"/>
<connect gate="G$1" pin="TDO" pad="C14"/>
<connect gate="G$1" pin="TEST" pad="N1"/>
<connect gate="G$1" pin="TMC" pad="E2"/>
<connect gate="G$1" pin="TMC1" pad="V3"/>
<connect gate="G$1" pin="TMC2" pad="E3"/>
<connect gate="G$1" pin="TMS" pad="A11"/>
<connect gate="G$1" pin="TRDY" pad="V5"/>
<connect gate="G$1" pin="TRST" pad="B14"/>
<connect gate="G$1" pin="USERI/LLOCKI" pad="D20"/>
<connect gate="G$1" pin="USERO/LLOCKO" pad="D19"/>
<connect gate="G$1" pin="VDD1_5_1" pad="C2"/>
<connect gate="G$1" pin="VDD1_5_236" pad="L1"/>
<connect gate="G$1" pin="VDD1_5_236@1" pad="L2"/>
<connect gate="G$1" pin="VDD1_5_236@2" pad="M1"/>
<connect gate="G$1" pin="VDD1_5_4" pad="D6"/>
<connect gate="G$1" pin="VDD1_5_5" pad="C13"/>
<connect gate="G$1" pin="VDD1_5_7" pad="C9"/>
<connect gate="G$1" pin="VDD1_5_8" pad="W5"/>
<connect gate="G$1" pin="VDD2_5_1" pad="C17"/>
<connect gate="G$1" pin="VDD2_5_2" pad="Y5"/>
<connect gate="G$1" pin="VDD2_5_3" pad="H18"/>
<connect gate="G$1" pin="VDD2_5_3@1" pad="J17"/>
<connect gate="G$1" pin="VDD2_5_4" pad="V9"/>
<connect gate="G$1" pin="VDD2_5_56" pad="T16"/>
<connect gate="G$1" pin="VDD2_5_56@1" pad="U15"/>
<connect gate="G$1" pin="VDD3_3" pad="D7"/>
<connect gate="G$1" pin="VDD3_3@1" pad="D8"/>
<connect gate="G$1" pin="VDD3_3@10" pad="F16"/>
<connect gate="G$1" pin="VDD3_3@11" pad="F17"/>
<connect gate="G$1" pin="VDD3_3@12" pad="G15"/>
<connect gate="G$1" pin="VDD3_3@13" pad="G16"/>
<connect gate="G$1" pin="VDD3_3@14" pad="H16"/>
<connect gate="G$1" pin="VDD3_3@15" pad="J16"/>
<connect gate="G$1" pin="VDD3_3@16" pad="K16"/>
<connect gate="G$1" pin="VDD3_3@17" pad="N16"/>
<connect gate="G$1" pin="VDD3_3@18" pad="P16"/>
<connect gate="G$1" pin="VDD3_3@19" pad="R16"/>
<connect gate="G$1" pin="VDD3_3@2" pad="D9"/>
<connect gate="G$1" pin="VDD3_3@20" pad="T12"/>
<connect gate="G$1" pin="VDD3_3@21" pad="T15"/>
<connect gate="G$1" pin="VDD3_3@22" pad="U10"/>
<connect gate="G$1" pin="VDD3_3@23" pad="U11"/>
<connect gate="G$1" pin="VDD3_3@24" pad="U14"/>
<connect gate="G$1" pin="VDD3_3@25" pad="V14"/>
<connect gate="G$1" pin="VDD3_3@3" pad="E5"/>
<connect gate="G$1" pin="VDD3_3@4" pad="E9"/>
<connect gate="G$1" pin="VDD3_3@5" pad="E15"/>
<connect gate="G$1" pin="VDD3_3@6" pad="E16"/>
<connect gate="G$1" pin="VDD3_3@7" pad="E17"/>
<connect gate="G$1" pin="VDD3_3@8" pad="F5"/>
<connect gate="G$1" pin="VDD3_3@9" pad="F15"/>
<connect gate="G$1" pin="VDD_P" pad="J2"/>
<connect gate="G$1" pin="VDD_R" pad="H3"/>
<connect gate="G$1" pin="VDD_T" pad="J4"/>
<connect gate="G$1" pin="VSS_C" pad="F4"/>
<connect gate="G$1" pin="VSS_P0" pad="H4"/>
<connect gate="G$1" pin="VSS_P1" pad="G4"/>
<connect gate="G$1" pin="VSS_R" pad="F1"/>
<connect gate="G$1" pin="VSS_RE" pad="G2"/>
<connect gate="G$1" pin="VSS_T" pad="K1"/>
<connect gate="G$1" pin="WAIT" pad="H17"/>
<connect gate="G$1" pin="WAKEIN" pad="B2"/>
<connect gate="G$1" pin="WAKEOUT" pad="D1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
