<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.1">
<drawing>
<library>
<description>&lt;b&gt;ROHM Co., Ltd.&lt;/b&gt; Semiconductor&lt;p&gt;
http://www.rohm.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOP8">
<description>&lt;b&gt;SOP8&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
</package>
<package name="HRP7">
<description>&lt;b&gt;HRP7&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
</package>
<package name="HSOP25">
<description>&lt;b&gt;HSOP 25&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
</package>
<package name="HSOP28">
<description>&lt;b&gt;HSOP-M28&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
</package>
<package name="EMT6">
<description>&lt;b&gt;General purpose transistors (dual transistors) EMX1 / UMX1N / IMX1&lt;/b&gt;&lt;p&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
</package>
<package name="UMT6">
<description>&lt;b&gt;UMT6 Package&lt;/b&gt; EIAJ: SC-88&lt;p&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
</package>
<package name="SMT6">
<description>&lt;b&gt;SMT6 Package&lt;/b&gt; EIAJ : SC-74&lt;p&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
</package>
</packages>
<symbols>
<symbol name="BD6230">
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="FIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BD6230HFP">
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="FIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="BD6230FP">
<pin name="OUT1@1" direction="out"/>
<pin name="OUT2@1" direction="out"/>
<pin name="FIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="OUT1@2" direction="out"/>
<pin name="OUT2@2" direction="out"/>
<pin name="RNF@1" direction="pas"/>
<pin name="RNF@2" direction="pas"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="BD6235FP">
<pin name="OUT1A" direction="out"/>
<pin name="OUT2A" direction="out"/>
<pin name="FINA" direction="in"/>
<pin name="RINA" direction="in"/>
<pin name="VREFA" direction="pas"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="RNFA" direction="pas"/>
<pin name="GND@3" direction="pwr"/>
<pin name="OUT1B" direction="out"/>
<pin name="OUT2B" direction="out"/>
<pin name="FINB" direction="in"/>
<pin name="RINB" direction="in"/>
<pin name="VREFB" direction="pas"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="RNFB" direction="pas"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="BD6220">
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="FIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BD6220HFP">
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="FIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BD623*F" prefix="IC">
<description>&lt;b&gt;H-bridge driver&lt;/b&gt; for brush motors&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
<gates>
<gate name="P" symbol="BD6230"/>
</gates>
<devices>
<device name="" package="SOP8">
<connects>
<connect gate="P" pin="FIN" pad="4"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="OUT1" pad="1"/>
<connect gate="P" pin="OUT2" pad="7"/>
<connect gate="P" pin="RIN" pad="5"/>
<connect gate="P" pin="VCC@1" pad="2"/>
<connect gate="P" pin="VCC@2" pad="3"/>
<connect gate="P" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BD6230F-E2"/>
<attribute name="OC_FARNELL" value="1716264"/>
<attribute name="OC_NEWARK" value="15R0529"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BD6231F-E2"/>
<attribute name="OC_FARNELL" value="1716265"/>
<attribute name="OC_NEWARK" value="15R0530"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD623*HFP" prefix="IC">
<description>&lt;b&gt;H-bridge driver&lt;/b&gt; for brush motors&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
<gates>
<gate name="P" symbol="BD6230HFP"/>
</gates>
<devices>
<device name="" package="HRP7">
<connects>
<connect gate="P" pin="FIN" pad="3"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="P"/>
<connect gate="P" pin="OUT1" pad="2"/>
<connect gate="P" pin="OUT2" pad="6"/>
<connect gate="P" pin="RIN" pad="5"/>
<connect gate="P" pin="VCC" pad="7"/>
<connect gate="P" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BD6231HFP-TR"/>
<attribute name="OC_FARNELL" value="1712946"/>
<attribute name="OC_NEWARK" value="24R5626"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BD6232HFP-TR"/>
<attribute name="OC_FARNELL" value="1712947"/>
<attribute name="OC_NEWARK" value="24R5627"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD6232FP" prefix="IC">
<description>&lt;b&gt;H-bridge driver&lt;/b&gt; for brush motors&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
<gates>
<gate name="G$1" symbol="BD6230FP"/>
</gates>
<devices>
<device name="" package="HSOP25">
<connects>
<connect gate="G$1" pin="FIN" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="GND@1"/>
<connect gate="G$1" pin="GND@3" pad="GND@2"/>
<connect gate="G$1" pin="OUT1@1" pad="1"/>
<connect gate="G$1" pin="OUT1@2" pad="2"/>
<connect gate="G$1" pin="OUT2@1" pad="12"/>
<connect gate="G$1" pin="OUT2@2" pad="13"/>
<connect gate="G$1" pin="RIN" pad="19"/>
<connect gate="G$1" pin="RNF@1" pad="7"/>
<connect gate="G$1" pin="RNF@2" pad="8"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="22"/>
<connect gate="G$1" pin="VCC@3" pad="23"/>
<connect gate="G$1" pin="VREF" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BD6232FP-E2"/>
<attribute name="OC_FARNELL" value="1716266"/>
<attribute name="OC_NEWARK" value="15R0531"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD623*FP" prefix="IC">
<description>&lt;b&gt;H-bridge driver&lt;/b&gt; for brush motors&lt;p&gt;
Source: http://www.rohm.com/products/databook/motor/pdf/bd623x_series-e.pdf</description>
<gates>
<gate name="G$1" symbol="BD6235FP"/>
</gates>
<devices>
<device name="" package="HSOP28">
<connects>
<connect gate="G$1" pin="FINA" pad="11"/>
<connect gate="G$1" pin="FINB" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="GND@1"/>
<connect gate="G$1" pin="GND@4" pad="GND@2"/>
<connect gate="G$1" pin="OUT1A" pad="1"/>
<connect gate="G$1" pin="OUT1B" pad="14"/>
<connect gate="G$1" pin="OUT2A" pad="6"/>
<connect gate="G$1" pin="OUT2B" pad="19"/>
<connect gate="G$1" pin="RINA" pad="10"/>
<connect gate="G$1" pin="RINB" pad="22"/>
<connect gate="G$1" pin="RNFA" pad="3"/>
<connect gate="G$1" pin="RNFB" pad="16"/>
<connect gate="G$1" pin="VCC@1" pad="24"/>
<connect gate="G$1" pin="VCC@2" pad="25"/>
<connect gate="G$1" pin="VCC@3" pad="12"/>
<connect gate="G$1" pin="VCC@4" pad="13"/>
<connect gate="G$1" pin="VREFA" pad="9"/>
<connect gate="G$1" pin="VREFB" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IMX1" prefix="T">
<description>&lt;b&gt;General purpose transistors (dual transistors)&lt;/b&gt; &lt;p&gt;
 Two 2SC2412K chips in a EMT or UMT or SMT package.&lt;br&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
<gates>
<gate name="A" symbol="NPN"/>
<gate name="B" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SMT6">
<connects>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="6"/>
<connect gate="B" pin="B" pad="2"/>
<connect gate="B" pin="C" pad="4"/>
<connect gate="B" pin="E" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="IMX1T110"/>
<attribute name="OC_FARNELL" value="1680348"/>
<attribute name="OC_NEWARK" value="74M2434"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UMX1N" prefix="Q">
<description>&lt;b&gt;General purpose transistors (dual transistors)&lt;/b&gt; &lt;p&gt;
 Two 2SC2412K chips in a EMT or UMT or SMT package.&lt;br&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
<gates>
<gate name="A" symbol="NPN"/>
<gate name="B" symbol="NPN"/>
</gates>
<devices>
<device name="" package="UMT6">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="6"/>
<connect gate="A" pin="E" pad="1"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="3"/>
<connect gate="B" pin="E" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UMX1NTN"/>
<attribute name="OC_FARNELL" value="1680410"/>
<attribute name="OC_NEWARK" value="40P3417"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EMX1" prefix="T">
<description>&lt;b&gt;General purpose transistors (dual transistors)&lt;/b&gt; &lt;p&gt;
 Two 2SC2412K chips in a EMT or UMT or SMT package.&lt;br&gt;
Source: http://www.rohm.com/products/databook/tr/pdf/umx1n.pdf</description>
<gates>
<gate name="A" symbol="NPN"/>
<gate name="B" symbol="NPN"/>
</gates>
<devices>
<device name="" package="EMT6">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="6"/>
<connect gate="A" pin="E" pad="1"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="3"/>
<connect gate="B" pin="E" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EMX1T2R"/>
<attribute name="OC_FARNELL" value="1680314"/>
<attribute name="OC_NEWARK" value="40P3026"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD6220" prefix="IC">
<description>&lt;b&gt;H-bridge drivers (18V max.)&lt;/b&gt;&lt;p&gt;
Source: http://www.farnell.com/datasheets/389117.pdf</description>
<gates>
<gate name="G$1" symbol="BD6220"/>
</gates>
<devices>
<device name="F" package="SOP8">
<connects>
<connect gate="G$1" pin="FIN" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="RIN" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="3"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD622*HFP" prefix="IC">
<description>&lt;b&gt;H-bridge drivers (18V max.)&lt;/b&gt;&lt;p&gt;
Source: http://www.farnell.com/datasheets/389117.pdf</description>
<gates>
<gate name="G$1" symbol="BD6220HFP"/>
</gates>
<devices>
<device name="" package="HRP7">
<connects>
<connect gate="G$1" pin="FIN" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 P" route="any"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="RIN" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="0"/>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
