<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="1.27" x2="17.78" y2="1.27" width="0" layer="20"/>
<wire x1="17.78" y1="1.27" x2="17.78" y2="16.51" width="0" layer="20"/>
<wire x1="17.78" y1="16.51" x2="1.27" y2="16.5" width="0" layer="20"/>
<wire x1="1.27" y1="16.5" x2="1.27" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="paolo">
<description>Paolo's Library</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SIP4">
</package>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; AVR ISP 10 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="paolo" package="C0805" value=""/>
<element name="IC1" library="atmel" package="8S2" value="TINY13-20SU">
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="96K6522"/>
<attribute name="OC_FARNELL" value="9171568"/>
</element>
<element name="JP1" library="avr-7" package="AVR-ISP-10" value="AVR-ISP-10"/>
<element name="JP2" library="paolo" package="SIP4" value=""/>
<element name="JP3" library="paolo" package="SIP4" value=""/>
<element name="LED1" library="paolo" package="SML0805" value=""/>
<element name="R1" library="paolo" package="M0805" value=""/>
<element name="R2" library="paolo" package="M0805" value=""/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="IC1" pad="5"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RES">
<contactref element="IC1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PB3">
<contactref element="IC1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="IC1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
