<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4.2">
<drawing>
<library>
<description>&lt;b&gt;APLUS INTEGRATED CIRCUITS INC.&lt;/b&gt;&lt;p&gt;
# Created by SCRIPT exported from Ultra Librarian Gold 5.3.88 Copyright © 1999-2010&lt;br&gt;
# Tanvir Mohammed, Premier Farnell&lt;br&gt;
2013-04-24 alf@cadsoft.de</description>
<packages>
<package name="DIP254P1525X550-28P">
<description>&lt;b&gt;# Created by Ultra Librarian Gold 5.3.88 Copyright © 1999-2010&lt;/b&gt;&lt;p&gt;
# Tanvir Mohammed, Premier Farnell&lt;br&gt;
Origin corrected by alf@cadsoft.de</description>
</package>
<package name="SOP50P1030X264-28N">
<description>&lt;b&gt;# Created by Ultra Librarian Gold 5.3.88 Copyright © 1999-2010&lt;/b&gt;&lt;p&gt;
# Tanvir Mohammed, Premier Farnell</description>
</package>
</packages>
<symbols>
<symbol name="APR9600_DIP-28">
<pin name="VCCD" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="/STROBE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="EXTCLK" direction="in"/>
<pin name="/RE" direction="in"/>
<pin name="ANA_IN" direction="in"/>
<pin name="OSCR" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="/M1_MESSAGE" direction="in"/>
<pin name="/M2_NEXT" direction="in"/>
<pin name="/M3" direction="in"/>
<pin name="/M4" direction="in"/>
<pin name="/M5" direction="in"/>
<pin name="/M6" direction="in"/>
<pin name="/M7_END" direction="in"/>
<pin name="/M8_OPTION" direction="in"/>
<pin name="VSSD" direction="pas"/>
<pin name="VSSA" direction="pas"/>
<pin name="/BUSY" direction="in"/>
<pin name="BE" direction="in"/>
<pin name="MICIN" direction="in"/>
<pin name="MICREF" direction="in"/>
<pin name="SP-" direction="out"/>
<pin name="SP+" direction="out"/>
<pin name="ANA_OUT" direction="out"/>
</symbol>
<symbol name="APR9600_SOP-28">
<pin name="VCCD" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="/STROBE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="MSEL2" direction="in"/>
<pin name="EXTCLK" direction="in"/>
<pin name="/RE" direction="in"/>
<pin name="ANA_IN" direction="in"/>
<pin name="OSCR" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="/M1" direction="in"/>
<pin name="/M2_NEXT" direction="in"/>
<pin name="/M3" direction="in"/>
<pin name="/M4" direction="in"/>
<pin name="/M5" direction="in"/>
<pin name="/M6" direction="in"/>
<pin name="/M7" direction="in"/>
<pin name="/M8" direction="in"/>
<pin name="VSSD" direction="pas"/>
<pin name="VSSA" direction="pas"/>
<pin name="/BUSY" direction="in"/>
<pin name="BE" direction="in"/>
<pin name="MICIN" direction="in"/>
<pin name="MICREF" direction="in"/>
<pin name="SP+" direction="out"/>
<pin name="SP-" direction="out"/>
<pin name="ANA_OUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="APR9600_DIP-28" prefix="U">
<description>&lt;b&gt;SINGLE-CHIP VOICE RECORDING &amp; PLAYBACK DEVICE FOR SINGLE 60 SECOND&lt;/b&gt;&lt;p&gt;
# Created by SCRIPT exported from Ultra Librarian Gold 5.3.88 Copyright © 1999-2010&lt;br&gt;
# Tanvir Mohammed, Premier Farnell&lt;br&gt;
2013-04-24 alf@cadsoft.de</description>
<gates>
<gate name="A" symbol="APR9600_DIP-28"/>
</gates>
<devices>
<device name="" package="DIP254P1525X550-28P">
<connects>
<connect gate="A" pin="/BUSY" pad="10"/>
<connect gate="A" pin="/CE" pad="23"/>
<connect gate="A" pin="/M1_MESSAGE" pad="1"/>
<connect gate="A" pin="/M2_NEXT" pad="2"/>
<connect gate="A" pin="/M3" pad="3"/>
<connect gate="A" pin="/M4" pad="4"/>
<connect gate="A" pin="/M5" pad="5"/>
<connect gate="A" pin="/M6" pad="6"/>
<connect gate="A" pin="/M7_END" pad="8"/>
<connect gate="A" pin="/M8_OPTION" pad="9"/>
<connect gate="A" pin="/RE" pad="27"/>
<connect gate="A" pin="/STROBE" pad="22"/>
<connect gate="A" pin="AGC" pad="19"/>
<connect gate="A" pin="ANA_IN" pad="20"/>
<connect gate="A" pin="ANA_OUT" pad="21"/>
<connect gate="A" pin="BE" pad="11"/>
<connect gate="A" pin="EXTCLK" pad="26"/>
<connect gate="A" pin="MICIN" pad="17"/>
<connect gate="A" pin="MICREF" pad="18"/>
<connect gate="A" pin="MSEL1" pad="24"/>
<connect gate="A" pin="MSEL2" pad="25"/>
<connect gate="A" pin="OSCR" pad="7"/>
<connect gate="A" pin="SP+" pad="14"/>
<connect gate="A" pin="SP-" pad="15"/>
<connect gate="A" pin="VCCA" pad="16"/>
<connect gate="A" pin="VCCD" pad="28"/>
<connect gate="A" pin="VSSA" pad="13"/>
<connect gate="A" pin="VSSD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="APR9600_DIP-28"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PACKAGE" value="DIP-28"/>
<attribute name="SUPPLIER" value="APLUS INTEGRATED CIRCUITS INC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APR9600_SOP-28" prefix="U">
<description>&lt;b&gt;SINGLE-CHIP VOICE RECORDING &amp; PLAYBACK DEVICE FOR SINGLE 60 SECOND&lt;/b&gt;&lt;p&gt;
# Created by SCRIPT exported from Ultra Librarian Gold 5.3.88 Copyright © 1999-2010&lt;br&gt;
# Tanvir Mohammed, Premier Farnell&lt;br&gt;
2013-04-24 alf@cadsoft.de</description>
<gates>
<gate name="A" symbol="APR9600_SOP-28"/>
</gates>
<devices>
<device name="" package="SOP50P1030X264-28N">
<connects>
<connect gate="A" pin="/BUSY" pad="17"/>
<connect gate="A" pin="/CE" pad="2"/>
<connect gate="A" pin="/M1" pad="8"/>
<connect gate="A" pin="/M2_NEXT" pad="9"/>
<connect gate="A" pin="/M3" pad="10"/>
<connect gate="A" pin="/M4" pad="11"/>
<connect gate="A" pin="/M5" pad="12"/>
<connect gate="A" pin="/M6" pad="13"/>
<connect gate="A" pin="/M7" pad="15"/>
<connect gate="A" pin="/M8" pad="16"/>
<connect gate="A" pin="/RE" pad="6"/>
<connect gate="A" pin="/STROBE" pad="1"/>
<connect gate="A" pin="AGC" pad="26"/>
<connect gate="A" pin="ANA_IN" pad="27"/>
<connect gate="A" pin="ANA_OUT" pad="28"/>
<connect gate="A" pin="BE" pad="18"/>
<connect gate="A" pin="EXTCLK" pad="5"/>
<connect gate="A" pin="MICIN" pad="24"/>
<connect gate="A" pin="MICREF" pad="25"/>
<connect gate="A" pin="MSEL1" pad="3"/>
<connect gate="A" pin="MSEL2" pad="4"/>
<connect gate="A" pin="OSCR" pad="14"/>
<connect gate="A" pin="SP+" pad="21"/>
<connect gate="A" pin="SP-" pad="22"/>
<connect gate="A" pin="VCCA" pad="23"/>
<connect gate="A" pin="VCCD" pad="7"/>
<connect gate="A" pin="VSSA" pad="20"/>
<connect gate="A" pin="VSSD" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="APR9600_SOP-28"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="APLUS INTEGRATED CIRCUITS INC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
