<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<library>
<description>C16 Cartridge Big</description>
<packages>
<package name="C16CART">
</package>
<package name="C16CART_SMALL">
</package>
</packages>
<symbols>
<symbol name="C16CART">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VDD"/>
<pin name="/IRQ"/>
<pin name="CR-/W"/>
<pin name="C1_H"/>
<pin name="C2_L"/>
<pin name="C2_H"/>
<pin name="/CS1"/>
<pin name="/CS0"/>
<pin name="/CAS"/>
<pin name="MUX"/>
<pin name="BA"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="AEC"/>
<pin name="EXAUD"/>
<pin name="PHI2"/>
<pin name="VSS"/>
<pin name="GND1"/>
<pin name="C1_L"/>
<pin name="/RESET"/>
<pin name="/RAS"/>
<pin name="PHI2_1"/>
<pin name="A15"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="VSS1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C16CARTRIDGE">
<gates>
<gate name="C16_CARTRIDGE" symbol="C16CART"/>
</gates>
<devices>
<device name="" package="C16CART">
<connects>
<connect gate="C16_CARTRIDGE" pin="/CAS" pad="11"/>
<connect gate="C16_CARTRIDGE" pin="/CS0" pad="10"/>
<connect gate="C16_CARTRIDGE" pin="/CS1" pad="9"/>
<connect gate="C16_CARTRIDGE" pin="/IRQ" pad="4"/>
<connect gate="C16_CARTRIDGE" pin="/RAS" pad="D"/>
<connect gate="C16_CARTRIDGE" pin="/RESET" pad="C"/>
<connect gate="C16_CARTRIDGE" pin="A0" pad="Y"/>
<connect gate="C16_CARTRIDGE" pin="A1" pad="X"/>
<connect gate="C16_CARTRIDGE" pin="A10" pad="M"/>
<connect gate="C16_CARTRIDGE" pin="A11" pad="L"/>
<connect gate="C16_CARTRIDGE" pin="A12" pad="K"/>
<connect gate="C16_CARTRIDGE" pin="A13" pad="J"/>
<connect gate="C16_CARTRIDGE" pin="A14" pad="H"/>
<connect gate="C16_CARTRIDGE" pin="A15" pad="F"/>
<connect gate="C16_CARTRIDGE" pin="A2" pad="W"/>
<connect gate="C16_CARTRIDGE" pin="A3" pad="V"/>
<connect gate="C16_CARTRIDGE" pin="A4" pad="U"/>
<connect gate="C16_CARTRIDGE" pin="A5" pad="T"/>
<connect gate="C16_CARTRIDGE" pin="A6" pad="S"/>
<connect gate="C16_CARTRIDGE" pin="A7" pad="R"/>
<connect gate="C16_CARTRIDGE" pin="A8" pad="P"/>
<connect gate="C16_CARTRIDGE" pin="A9" pad="N"/>
<connect gate="C16_CARTRIDGE" pin="AEC" pad="22"/>
<connect gate="C16_CARTRIDGE" pin="BA" pad="13"/>
<connect gate="C16_CARTRIDGE" pin="C1_H" pad="6"/>
<connect gate="C16_CARTRIDGE" pin="C1_L" pad="B"/>
<connect gate="C16_CARTRIDGE" pin="C2_H" pad="8"/>
<connect gate="C16_CARTRIDGE" pin="C2_L" pad="7"/>
<connect gate="C16_CARTRIDGE" pin="CR-/W" pad="5"/>
<connect gate="C16_CARTRIDGE" pin="D0" pad="21"/>
<connect gate="C16_CARTRIDGE" pin="D1" pad="20"/>
<connect gate="C16_CARTRIDGE" pin="D2" pad="19"/>
<connect gate="C16_CARTRIDGE" pin="D3" pad="18"/>
<connect gate="C16_CARTRIDGE" pin="D4" pad="17"/>
<connect gate="C16_CARTRIDGE" pin="D5" pad="16"/>
<connect gate="C16_CARTRIDGE" pin="D6" pad="15"/>
<connect gate="C16_CARTRIDGE" pin="D7" pad="14"/>
<connect gate="C16_CARTRIDGE" pin="EXAUD" pad="23"/>
<connect gate="C16_CARTRIDGE" pin="GND" pad="1"/>
<connect gate="C16_CARTRIDGE" pin="GND1" pad="A"/>
<connect gate="C16_CARTRIDGE" pin="MUX" pad="12"/>
<connect gate="C16_CARTRIDGE" pin="NC1" pad="Z"/>
<connect gate="C16_CARTRIDGE" pin="NC2" pad="AA"/>
<connect gate="C16_CARTRIDGE" pin="NC3" pad="BB"/>
<connect gate="C16_CARTRIDGE" pin="PHI2" pad="24"/>
<connect gate="C16_CARTRIDGE" pin="PHI2_1" pad="E"/>
<connect gate="C16_CARTRIDGE" pin="VCC" pad="2"/>
<connect gate="C16_CARTRIDGE" pin="VDD" pad="3"/>
<connect gate="C16_CARTRIDGE" pin="VSS" pad="25"/>
<connect gate="C16_CARTRIDGE" pin="VSS1" pad="CC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="C16CART_SMALL">
<connects>
<connect gate="C16_CARTRIDGE" pin="/CAS" pad="11"/>
<connect gate="C16_CARTRIDGE" pin="/CS0" pad="10"/>
<connect gate="C16_CARTRIDGE" pin="/CS1" pad="9"/>
<connect gate="C16_CARTRIDGE" pin="/IRQ" pad="4"/>
<connect gate="C16_CARTRIDGE" pin="/RAS" pad="D"/>
<connect gate="C16_CARTRIDGE" pin="/RESET" pad="C"/>
<connect gate="C16_CARTRIDGE" pin="A0" pad="Y"/>
<connect gate="C16_CARTRIDGE" pin="A1" pad="X"/>
<connect gate="C16_CARTRIDGE" pin="A10" pad="M"/>
<connect gate="C16_CARTRIDGE" pin="A11" pad="L"/>
<connect gate="C16_CARTRIDGE" pin="A12" pad="K"/>
<connect gate="C16_CARTRIDGE" pin="A13" pad="J"/>
<connect gate="C16_CARTRIDGE" pin="A14" pad="H"/>
<connect gate="C16_CARTRIDGE" pin="A15" pad="F"/>
<connect gate="C16_CARTRIDGE" pin="A2" pad="W"/>
<connect gate="C16_CARTRIDGE" pin="A3" pad="V"/>
<connect gate="C16_CARTRIDGE" pin="A4" pad="U"/>
<connect gate="C16_CARTRIDGE" pin="A5" pad="T"/>
<connect gate="C16_CARTRIDGE" pin="A6" pad="S"/>
<connect gate="C16_CARTRIDGE" pin="A7" pad="R"/>
<connect gate="C16_CARTRIDGE" pin="A8" pad="P"/>
<connect gate="C16_CARTRIDGE" pin="A9" pad="N"/>
<connect gate="C16_CARTRIDGE" pin="AEC" pad="22"/>
<connect gate="C16_CARTRIDGE" pin="BA" pad="13"/>
<connect gate="C16_CARTRIDGE" pin="C1_H" pad="6"/>
<connect gate="C16_CARTRIDGE" pin="C1_L" pad="B"/>
<connect gate="C16_CARTRIDGE" pin="C2_H" pad="8"/>
<connect gate="C16_CARTRIDGE" pin="C2_L" pad="7"/>
<connect gate="C16_CARTRIDGE" pin="CR-/W" pad="5"/>
<connect gate="C16_CARTRIDGE" pin="D0" pad="21"/>
<connect gate="C16_CARTRIDGE" pin="D1" pad="20"/>
<connect gate="C16_CARTRIDGE" pin="D2" pad="19"/>
<connect gate="C16_CARTRIDGE" pin="D3" pad="18"/>
<connect gate="C16_CARTRIDGE" pin="D4" pad="17"/>
<connect gate="C16_CARTRIDGE" pin="D5" pad="16"/>
<connect gate="C16_CARTRIDGE" pin="D6" pad="15"/>
<connect gate="C16_CARTRIDGE" pin="D7" pad="14"/>
<connect gate="C16_CARTRIDGE" pin="EXAUD" pad="23"/>
<connect gate="C16_CARTRIDGE" pin="GND" pad="1"/>
<connect gate="C16_CARTRIDGE" pin="GND1" pad="A"/>
<connect gate="C16_CARTRIDGE" pin="MUX" pad="12"/>
<connect gate="C16_CARTRIDGE" pin="NC1" pad="Z"/>
<connect gate="C16_CARTRIDGE" pin="NC2" pad="AA"/>
<connect gate="C16_CARTRIDGE" pin="NC3" pad="BB"/>
<connect gate="C16_CARTRIDGE" pin="PHI2" pad="24"/>
<connect gate="C16_CARTRIDGE" pin="PHI2_1" pad="E"/>
<connect gate="C16_CARTRIDGE" pin="VCC" pad="2"/>
<connect gate="C16_CARTRIDGE" pin="VDD" pad="3"/>
<connect gate="C16_CARTRIDGE" pin="VSS" pad="25"/>
<connect gate="C16_CARTRIDGE" pin="VSS1" pad="CC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
