<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;XMULTIPLE&lt;/b&gt; Connector&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="XRJF-01A-0-D2A-010">
<description>&lt;b&gt;RC45&lt;/b&gt; without LED, schielded, with transformer, side entry PCB Jack&lt;p&gt;
Source: XRJF-01A-0-D2A-010(01).pdf</description>
</package>
<package name="XRJK-S-01-6-4-0-9M2">
<description>&lt;b&gt;RJ11 Connector&lt;/b&gt; without LED, 6 position, 4 contacts, shielded, thrue hole&lt;p&gt;
Source: XRJK-S-01-6-4-0-9M2(01).pdf</description>
</package>
<package name="XRJK-S-01-6-6-0-2G2-NO">
<description>&lt;b&gt;RJ11 Connector&lt;/b&gt; without LED, 6 position, 6 contacts, shielded, thrue hole&lt;p&gt;
Source: XRJK-S-01-6-6-0-2G2-NO(01).pdf</description>
</package>
</packages>
<symbols>
<symbol name="RJ45-8-SHIELD">
<pin name="S@2" direction="pas"/>
<pin name="S@1" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="RJ11-4-SHIELD">
<pin name="S@2" direction="pas"/>
<pin name="S@1" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="RJ11-6-SHIELD">
<pin name="S@2" direction="pas"/>
<pin name="S@1" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="XRJF" prefix="X">
<description>&lt;b&gt;RC45&lt;/b&gt; schielded, without LED, with transformer, side entry PCB Jack&lt;p&gt;
Source: XRJF-01A-0-D2A-010(01).pdf</description>
<gates>
<gate name="G$1" symbol="RJ45-8-SHIELD"/>
</gates>
<devices>
<device name="" package="XRJF-01A-0-D2A-010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="S@1" pad="S1"/>
<connect gate="G$1" pin="S@2" pad="S2"/>
</connects>
<technologies>
<technology name="-01A-0-D22-020"/>
<technology name="-01A-0-D23-010"/>
<technology name="-01A-0-D2A-010"/>
<technology name="F-01A-0-D22-010"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XRJK*4" prefix="X">
<description>&lt;b&gt;RJ11 Connector&lt;/b&gt; without LED, 6 position, 4 contacts, thrue hole&lt;p&gt;
Source: XRJK-S-01-6-4-0-9M2(01).pdf</description>
<gates>
<gate name="G$1" symbol="RJ11-4-SHIELD"/>
</gates>
<devices>
<device name="-0-9M2" package="XRJK-S-01-6-4-0-9M2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="S@1" pad="S1"/>
<connect gate="G$1" pin="S@2" pad="S2"/>
</connects>
<technologies>
<technology name="-S-01-6-"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XRJK*6" prefix="X">
<description>&lt;b&gt;RJ11 Connector&lt;/b&gt; without LED, 6 position, 6 contacts, shielded, thrue hole&lt;p&gt;
Source: XRJK-S-01-6-6-0-2G2-NO(01).pdf</description>
<gates>
<gate name="G$1" symbol="RJ11-6-SHIELD"/>
</gates>
<devices>
<device name="-0-2G2-NO" package="XRJK-S-01-6-6-0-2G2-NO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="S@1" pad="S1"/>
<connect gate="G$1" pin="S@2" pad="S2"/>
</connects>
<technologies>
<technology name="-S-01-6-"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
