<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>LT-Spice library generated with :&lt;br&gt;
import-ltspice.ulp&lt;br&gt;
from: E:/Programme/LTC/LTspiceIV/lib/sym/Misc/*.asy&lt;br&gt;
at 12.06.2012 10:26:07
&lt;p&gt;
2N5458.DEV&lt;br&gt;
2N7002.DEV&lt;br&gt;
BATTERY.DEV&lt;br&gt;
CELL.DEV&lt;br&gt;
DIAC.DEV&lt;br&gt;
DIP8.DEV&lt;br&gt;
DIP10.DEV&lt;br&gt;
DIP14.DEV&lt;br&gt;
DIP16.DEV&lt;br&gt;
DIP20.DEV&lt;br&gt;
EPOLY.DEV&lt;br&gt;
EUROPEANCAP.DEV&lt;br&gt;
EUROPEANPOLCAP.DEV&lt;br&gt;
EUROPEANRESISTOR.DEV&lt;br&gt;
FIXEDIND.DEV&lt;br&gt;
JUMPER.DEV&lt;br&gt;
NE555.DEV&lt;br&gt;
NEONBULB.DEV&lt;br&gt;
NIGBT.DEV&lt;br&gt;
PENTODE.DEV&lt;br&gt;
PIGBT.DEV&lt;br&gt;
SCR.DEV&lt;br&gt;
TETRODE.DEV&lt;br&gt;
TOWTOM2.DEV&lt;br&gt;
TRIAC.DEV&lt;br&gt;
TRIODE.DEV&lt;br&gt;
URC.DEV&lt;br&gt;
URC2.DEV&lt;br&gt;
XTAL.DEV&lt;br&gt;
XVARISTOR.DEV&lt;br&gt;</description>
<packages>
<package name="BR210S">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead molded, vertical</description>
</package>
<package name="BR220S">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
3-lead molded, vertical</description>
</package>
<package name="05">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TOWTOM2">
<description>Dummy</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="3V60R">
<description>&lt;b&gt;NC ACCU&lt;/b&gt; Varta</description>
</package>
</packages>
<symbols>
<symbol name="N_CHANNEL_TRANSISTOR">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BATTERY">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="CELL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DIAC">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DIP10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="DIP14">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="DIP16">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="DIP20">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="DIP8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="EPOLY">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="EUROPEANCAP">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="EUROPEANPOLCAP">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="EUROPEANRESISTOR">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="FIXEDIND">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="JUMPER">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="NE555">
<pin name="GND" direction="pas"/>
<pin name="TRIG" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="RST" direction="pas"/>
<pin name="CV" direction="pas"/>
<pin name="THRS" direction="pas"/>
<pin name="DIS" direction="pas"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="NEONBULB">
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
</symbol>
<symbol name="NIGBT">
<pin name="C" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="PENTODE">
<pin name="CATHODE" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="G3" direction="pas"/>
<pin name="ANODE" direction="pas"/>
</symbol>
<symbol name="PIGBT">
<pin name="C" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="SCR">
<pin name="A" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="TETRODE">
<pin name="ANODE" direction="pas"/>
<pin name="SCREEN" direction="pas"/>
<pin name="GRID" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="TOWTOM2">
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="INV" direction="pas"/>
</symbol>
<symbol name="TRIAC">
<pin name="MT2" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="MT1" direction="pas"/>
</symbol>
<symbol name="TRIODE">
<pin name="PLATE" direction="pas"/>
<pin name="GRID" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="URC">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="URC2">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="XTAL">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="XVARISTOR">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2N7002" prefix="X">
<description>Small signal N-Channel MOSFET transistor</description>
<gates>
<gate name="G$1" symbol="N_CHANNEL_TRANSISTOR"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="2N7002.mod"/>
<attribute name="VALUE2" value=" 2N7002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="V">
<description>Voltage Source, either DC, AC, PULSE, SINE, PWL, EXP, or SFFM</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="" package="3V60R">
<connects>
<connect gate="G$1" pin="+" pad="+ +@1" route="any"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CELL" prefix="V">
<description>Voltage Source, either DC, AC, PULSE, SINE, PWL, EXP, or SFFM</description>
<gates>
<gate name="G$1" symbol="CELL"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIAC" prefix="X">
<description>Generic Bi-directional Trigger Device symbol for use with a model that you supply</description>
<gates>
<gate name="G$1" symbol="DIAC"/>
</gates>
<devices>
<device name="" package="BR210S">
<connects>
<connect gate="G$1" pin="+" pad="T1"/>
<connect gate="G$1" pin="-" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP10" prefix="X" uservalue="yes">
<description>Generic Symbol for use with subcircuts that you supply.</description>
<gates>
<gate name="G$1" symbol="DIP10"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP14" prefix="X" uservalue="yes">
<description>Generic Symbol for use with subcircuts that you supply.</description>
<gates>
<gate name="G$1" symbol="DIP14"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP16" prefix="X" uservalue="yes">
<description>Generic Symbol for use with subcircuts that you supply.</description>
<gates>
<gate name="G$1" symbol="DIP16"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP20" prefix="X" uservalue="yes">
<description>Generic Symbol for use with subcircuts that you supply.</description>
<gates>
<gate name="G$1" symbol="DIP20"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP8" prefix="X" uservalue="yes">
<description>Generic Symbol for use with subcircuts that you supply.</description>
<gates>
<gate name="G$1" symbol="DIP8"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPOLY" prefix="E">
<description>Voltage dependent voltage source with two terminals.  Useful for drafting schematic generating archaic voltage controlled syntax.</description>
<gates>
<gate name="G$1" symbol="EPOLY"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPEANCAP" prefix="C">
<description>Polarized Capacitor</description>
<gates>
<gate name="G$1" symbol="EUROPEANCAP"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPEANPOLCAP" prefix="C">
<description>Polarized Capacitor</description>
<gates>
<gate name="G$1" symbol="EUROPEANPOLCAP"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPEANRESISTOR" prefix="R">
<description>A Resistor(European style graphic)</description>
<gates>
<gate name="G$1" symbol="EUROPEANRESISTOR"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIXEDIND" prefix="L">
<description>An inductor that cannot be edited.  Typically used with the 1533/1534</description>
<gates>
<gate name="G$1" symbol="FIXEDIND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="DEFSUBSTRATE" value="noedit"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER" prefix="J" uservalue="yes">
<description>A wire jumper.  This component lets you give the same net two different names</description>
<gates>
<gate name="G$1" symbol="JUMPER"/>
</gates>
<devices>
<device name="" package="05">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555" prefix="X">
<description>An idealized 555 timer model.</description>
<gates>
<gate name="A" symbol="NE555"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="A" pin="CV" pad="5"/>
<connect gate="A" pin="DIS" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="RST" pad="4"/>
<connect gate="A" pin="THRS" pad="6"/>
<connect gate="A" pin="TRIG" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NEONBULB" prefix="X" uservalue="yes">
<description>Parameterized Neon Bulb</description>
<gates>
<gate name="G$1" symbol="NEONBULB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="MODELFILE" value="neonbulb.sub"/>
<attribute name="SPICELINE" value=" Zon=2K Ihold=200u"/>
<attribute name="SPICELINE2" value=" Tau=100u"/>
<attribute name="SPICEMODEL" value="neonbulb"/>
<attribute name="VALUE2" value=" Vstrike=100 Vhold=50"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NIGBT" prefix="X">
<description>N-Channel IBGT symbol for a model you supply.</description>
<gates>
<gate name="G$1" symbol="NIGBT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PENTODE" prefix="X">
<description>This symbol is for use with a subcircuit macromodel that you supply.</description>
<gates>
<gate name="G$1" symbol="PENTODE"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIGBT" prefix="X">
<description>P-Channel IBGT symbol for a model you supply.</description>
<gates>
<gate name="G$1" symbol="PIGBT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCR" prefix="X">
<description>Generic SCR symbol for use with a model that you supply.</description>
<gates>
<gate name="G$1" symbol="SCR"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TETRODE" prefix="X">
<description>This symbol is for use with a subcircuit macromodel that you supply.</description>
<gates>
<gate name="G$1" symbol="TETRODE"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOWTOM2" prefix="X">
<description>2nd Order Tow-Thomas Filter building block.  Needs .lib TowTom2.sub &amp; .params R=10K C=160p GBW1=10Meg GBW2=15Meg Aol=100K</description>
<gates>
<gate name="G$1" symbol="TOWTOM2"/>
</gates>
<devices>
<device name="" package="TOWTOM2">
<connects>
<connect gate="G$1" pin="INV" pad="G$1INV"/>
<connect gate="G$1" pin="V1" pad="G$1V1"/>
<connect gate="G$1" pin="V2" pad="G$1V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIAC" prefix="X">
<description>Generic TRIAC symbol for use with a model that you supply.</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="" package="BR220S">
<connects>
<connect gate="G$1" pin="G" pad="T1"/>
<connect gate="G$1" pin="MT1" pad="T2"/>
<connect gate="G$1" pin="MT2" pad="T3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIODE" prefix="X">
<description>This symbol is for use with a subcircuit macromodel that you supply.</description>
<gates>
<gate name="G$1" symbol="TRIODE"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="URC" prefix="U">
<description>Uniform RC-line.  Intended for interconnection on IC s but rarely used.'</description>
<gates>
<gate name="G$1" symbol="URC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="URC2" prefix="U">
<description>Uniform RC-line.  Intended for interconnection on IC s but rarely used.'</description>
<gates>
<gate name="G$1" symbol="URC2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL" prefix="C">
<description>Piezoelectric crystal.  Set C, Lser and Cpar to set series and parallel resonances.  This is actually the same as a capacitor.</description>
<gates>
<gate name="G$1" symbol="XTAL"/>
</gates>
<devices>
<device name="" package="HC49UP">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XVARISTOR" prefix="X">
<description>Generic varistor symbol for use with a model that you supply.</description>
<gates>
<gate name="G$1" symbol="XVARISTOR"/>
</gates>
<devices>
<device name="" package="BR210S">
<connects>
<connect gate="G$1" pin="A" pad="T1"/>
<connect gate="G$1" pin="B" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N5458" prefix="X">
<description>&lt;b&gt;N-Channel General Purpose Amplifier&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/46943.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="N_CHANNEL_TRANSISTOR"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
