<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;Supertex inc.&lt;/b&gt;&lt;p&gt;
www.supertex.com&lt;b&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOIC-16NG">
<description>&lt;b&gt;16-Lead SOIC (Narrow Body) Package Outline (NG)&lt;/b&gt;&lt;p&gt;
9.90x3.90mm body, 1.75mm height (max), 1.27mm pitch&lt;br&gt;
Source: www.supertex.com .. led_driver_ics_SG.pdf</description>
</package>
<package name="SOIC-08LG">
<description>&lt;b&gt;8-Lead SOIC (Narrow Body) Package Outline (LG)&lt;/b&gt;&lt;p&gt;
4.9x3.9mm body, 1.75mm height (max), 1.27mm pitch&lt;br&gt;
Source: www.supertex.com .. led_driver_ics_SG.pdf</description>
</package>
</packages>
<symbols>
<symbol name="HV9910B">
<pin name="VIN" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="GATE" direction="out"/>
<pin name="PWMD" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="LD" direction="in"/>
<pin name="RT" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HV9910B" prefix="IC">
<description>&lt;b&gt;Universal High Brightness LED Driver&lt;/b&gt;&lt;p&gt;
Source: www.supertex.com .. led_driver_ics_SG.pdf</description>
<gates>
<gate name="G$1" symbol="HV9910B"/>
</gates>
<devices>
<device name="LG" package="SOIC-08LG">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="GATE" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LD" pad="7"/>
<connect gate="G$1" pin="PWMD" pad="5"/>
<connect gate="G$1" pin="RT" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MXHV9910B"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15R9731"/>
</technology>
</technologies>
</device>
<device name="NG" package="SOIC-16NG">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GATE" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LD" pad="13"/>
<connect gate="G$1" pin="PWMD" pad="9"/>
<connect gate="G$1" pin="RT" pad="14"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
