<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="A68-A31">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Siemens, distributor Buerklin, 11G766</description>
</package>
<package name="9070-1W">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
 Marquardt</description>
</package>
<package name="9070-2W">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
 Marquardt</description>
</package>
<package name="316-917">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor RS Components</description>
</package>
<package name="316-923">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor RS Components</description>
</package>
<package name="320-916">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
distributor RS Components</description>
</package>
<package name="320-938">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
distributor RS Components</description>
</package>
<package name="M9040P">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
<package name="M9040P2">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
<package name="LPV-1">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;</description>
</package>
<package name="255SB">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
distributor Buerklin, 11G810</description>
</package>
<package name="M251">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor Buerklin, 11G702</description>
</package>
<package name="MS243">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;</description>
</package>
<package name="ITT-RT112">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
</package>
<package name="ITT-RT206">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
</package>
<package name="CK10">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
</package>
<package name="ITT-RT">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
</package>
<package name="ITT-RTBCD">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
</package>
<package name="CK101X12">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
</package>
<package name="CK102X06">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
</package>
<package name="CK103X04">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
</package>
<package name="CK104X03">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
</package>
<package name="REKN">
<description>&lt;b&gt;PUSH SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon-Cannon</description>
</package>
<package name="MARQ6425">
<description>&lt;b&gt;DIL SWITCH&lt;/b&gt;&lt;p&gt;
with LED, Marquardt</description>
</package>
<package name="RDT1034">
<description>&lt;b&gt;PUSH SWITCH&lt;/b&gt;&lt;p&gt;
www.radiohm.com</description>
</package>
<package name="SKHMPXE010">
<description>&lt;b&gt;6.2 X 6.5mm TACT Switch (SMD)&lt;/b&gt;&lt;p&gt;
Source: http://www3.alps.co.jp/WebObjects/catalog.woa/PDF/E/Switch/Tact/SKHM/SKHM.PDF</description>
</package>
<package name="SSRM1C6200">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM1C5400">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM-4">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM254700">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM263700">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM262400">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM264300">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM265900">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM342800">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="SRRM433700">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: SRRM.pdf</description>
</package>
<package name="ELMA-01-1X12">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-1X10MA">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
</package>
<package name="ELMA-01-1X11">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-1X10OA">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-2X6">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-4X3">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-1X6">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
</package>
<package name="ELMA-01-2X3">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="ELMA-01-4X2">
<description>&lt;b&gt;ELMA Rotary Switsh Type 01&lt;/b&gt;&lt;p&gt;
Source: rotary_switches_type_01_001.pdf</description>
</package>
<package name="71BT-30-A1">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 30°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-36-A1">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 36°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-36-A2">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 36°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-30-A2">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 30°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-30-AB1">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 30°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-36-AB1">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 36°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-36-AB2">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 36°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="71BT-30-AB2">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt; 30°&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
</package>
<package name="75AP36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75AF36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75BP36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75CP36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75BF36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75CF36">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75AF36-2">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75AP36-2">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75BF36-2">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75BP36-2">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="75CF36-2">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
</package>
<package name="50-1POLE22,5">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches one pole 22.5°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="50-2POLE22,5">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches two pole 22.5°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="50-1POLE30">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches one pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="50-2POLE30">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches two pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="50-3POLE30">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches three pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="50-4POLE30">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches four pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
</package>
<package name="24-1POLE36">
<description>&lt;b&gt;SERIES 24&lt;/b&gt; Rotary Switches one pole 36°&lt;p&gt;
Source: www.grayhill.com .. J-28.pdf</description>
</package>
<package name="TL3XPO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL4XPO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL3XYO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL4XYO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL3XWO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL4XWO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
<package name="TL1105">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TLE1105">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt; (EARTH TERMINAL)&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TL1105T">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TL1105SP">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TL1105JA">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TL1105J">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TL1105L-4,3">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="5501">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt;&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="5501-1LED">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt; with 1 LED&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="5501-2LED">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt; with 2 LED (red, green)&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="5511-2LED">
<description>&lt;b&gt;PUSHBUTTON SERIES 5511 SWITCHES&lt;/b&gt; with 2 LED (red, yellow)&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="5511-1LED">
<description>&lt;b&gt;PUSHBUTTON SERIES 5511 SWITCHES&lt;/b&gt; with 1 LED&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="5511">
<description>&lt;b&gt;PUSHBUTTON SERIES 5511 SWITCHES&lt;/b&gt;&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="2P2T">
</package>
<package name="3PDT">
<description>&lt;b&gt;3PDT 9 pin footswitch&lt;/b&gt; SF17020F-0302-21R-L&lt;p&gt;
Source: 3PDT.jpg</description>
</package>
</packages>
<symbols>
<symbol name="S">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="S+V">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="K" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="DS-U">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="KS-U">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SS-U">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="U">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="U2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SIS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="KS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DS-U-DU">
</symbol>
<symbol name="DS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="KS-DU">
</symbol>
<symbol name="KS-U-DU">
</symbol>
<symbol name="SS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SS-DU">
</symbol>
<symbol name="SS-U-DU">
</symbol>
<symbol name="DS-112">
<pin name="1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="C@" direction="pas"/>
</symbol>
<symbol name="DS-206">
<pin name="11" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="DS-BCD">
<pin name="1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="1/" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="2/" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="4/" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="8/" direction="pas"/>
<pin name="C@" direction="pas"/>
</symbol>
<symbol name="DS-A304">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DS-A112">
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="DS-A206">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="C6" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DS-A403">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="KS-UB">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="B1" direction="pas"/>
</symbol>
<symbol name="SIS-">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="KS-UB-">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="B1" direction="pas"/>
</symbol>
<symbol name="KS-U-">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="NORMOPEN">
<pin name="0@A" direction="pas"/>
<pin name="0@B" direction="pas"/>
<pin name="1@B" direction="pas"/>
<pin name="1@A" direction="pas"/>
</symbol>
<symbol name="DS-DU">
</symbol>
<symbol name="NORMOPEN2-1">
<pin name="A" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="NORMOPEN_SHIELD">
<pin name="1.1" direction="pas"/>
<pin name="1.2" direction="pas"/>
<pin name="2.2" direction="pas"/>
<pin name="2.1" direction="pas"/>
<pin name="SH" direction="pas"/>
</symbol>
<symbol name="DS-205">
<pin name="11" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="C2" direction="pas"/>
</symbol>
<symbol name="SSRM-4-1">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="SSRM-4-2">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="DS-106">
<pin name="1" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="DS-110">
<pin name="1" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="DS-111">
<pin name="1" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="DS-A203">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="DS-A402">
<pin name="A1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="DS-116">
<pin name="1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="DS-208">
<pin name="11" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="71" direction="pas"/>
<pin name="81" direction="pas"/>
<pin name="72" direction="pas"/>
<pin name="82" direction="pas"/>
</symbol>
<symbol name="ON-OFF-ON">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="MOM-OFF-MOM">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="ON-OFF-MOM">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="ON-MOM">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="MOM-OFF-MOM_2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="ON-MOM_2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="ON-OFF-MOM_2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="ON-OFF-ON_2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="U_2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="NO-NC-2">
<pin name="1A" direction="pas"/>
<pin name="1B" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="2P2T">
<pin name="1.1" direction="pas"/>
<pin name="2.1" direction="pas"/>
<pin name="3.1" direction="pas"/>
<pin name="1.2" direction="pas"/>
<pin name="2.2" direction="pas"/>
<pin name="3.2" direction="pas"/>
</symbol>
<symbol name="U_3L">
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="O2" direction="pas"/>
<pin name="P3" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="O3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="A68-A31" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Siemens, distributor Buerklin, 11G766</description>
<gates>
<gate name="B" symbol="U2"/>
<gate name="A" symbol="SIS-"/>
</gates>
<devices>
<device name="" package="A68-A31">
<connects>
<connect gate="A" pin="O" pad="1"/>
<connect gate="A" pin="P" pad="2"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="B" pin="P" pad="5"/>
<connect gate="B" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="320-916" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
distributor RS Components</description>
<gates>
<gate name="1" symbol="KS-U"/>
</gates>
<devices>
<device name="" package="320-916">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M9040P" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
<gates>
<gate name="1" symbol="KS-U"/>
</gates>
<devices>
<device name="" package="M9040P">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="316-917" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor RS Components</description>
<gates>
<gate name="1" symbol="KS-UB"/>
</gates>
<devices>
<device name="" package="316-917">
<connects>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="B1" pad="B1"/>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="316-923" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor RS Components</description>
<gates>
<gate name="B" symbol="U2"/>
<gate name="2" symbol="KS-UB-"/>
</gates>
<devices>
<device name="" package="316-923">
<connects>
<connect gate="2" pin="B" pad="B"/>
<connect gate="2" pin="B1" pad="B1"/>
<connect gate="2" pin="O" pad="1"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="B" pin="P" pad="5"/>
<connect gate="B" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="320-938" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
distributor RS Components</description>
<gates>
<gate name="B" symbol="U2"/>
<gate name="1" symbol="KS-U-"/>
</gates>
<devices>
<device name="" package="320-938">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="B" pin="P" pad="5"/>
<connect gate="B" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M9040P2" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
<gates>
<gate name="2" symbol="U2"/>
<gate name="1" symbol="KS-U-"/>
</gates>
<devices>
<device name="" package="M9040P2">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
<connect gate="2" pin="O" pad="4"/>
<connect gate="2" pin="P" pad="5"/>
<connect gate="2" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="255SB" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Distributor Buerklin, 11G810</description>
<gates>
<gate name="1" symbol="SIS"/>
</gates>
<devices>
<device name="" package="255SB">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV-1" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="KS-UB"/>
</gates>
<devices>
<device name="" package="LPV-1">
<connects>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="B1" pad="B1"/>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M251" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor Buerklin, 11G702</description>
<gates>
<gate name="1" symbol="SIS"/>
</gates>
<devices>
<device name="" package="M251">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MS243" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="KS"/>
</gates>
<devices>
<device name="" package="MS243">
<connects>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CK101X12" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
<gates>
<gate name="1" symbol="DS-A112"/>
</gates>
<devices>
<device name="" package="CK101X12">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
<connect gate="1" pin="A" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CK102X06" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
<gates>
<gate name="1" symbol="DS-A206"/>
</gates>
<devices>
<device name="" package="CK102X06">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="A1" pad="A1"/>
<connect gate="1" pin="A2" pad="A2"/>
<connect gate="1" pin="A3" pad="A3"/>
<connect gate="1" pin="A4" pad="A4"/>
<connect gate="1" pin="A5" pad="A5"/>
<connect gate="1" pin="A6" pad="A6"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="C1" pad="C1"/>
<connect gate="1" pin="C2" pad="C2"/>
<connect gate="1" pin="C3" pad="C3"/>
<connect gate="1" pin="C4" pad="C4"/>
<connect gate="1" pin="C5" pad="C5"/>
<connect gate="1" pin="C6" pad="C6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CK103X04" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
<gates>
<gate name="1" symbol="DS-A304"/>
</gates>
<devices>
<device name="" package="CK103X04">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="A1" pad="A1"/>
<connect gate="1" pin="A2" pad="A2"/>
<connect gate="1" pin="A3" pad="A3"/>
<connect gate="1" pin="A4" pad="A4"/>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="B1" pad="B1"/>
<connect gate="1" pin="B2" pad="B2"/>
<connect gate="1" pin="B3" pad="B3"/>
<connect gate="1" pin="B4" pad="B4"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="C1" pad="C1"/>
<connect gate="1" pin="C2" pad="C2"/>
<connect gate="1" pin="C3" pad="C3"/>
<connect gate="1" pin="C4" pad="C4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CK104X03" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
<gates>
<gate name="1" symbol="DS-A403"/>
</gates>
<devices>
<device name="" package="CK104X03">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="A1" pad="A1"/>
<connect gate="1" pin="A2" pad="A2"/>
<connect gate="1" pin="A3" pad="A3"/>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="B1" pad="B1"/>
<connect gate="1" pin="B2" pad="B2"/>
<connect gate="1" pin="B3" pad="B3"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="C1" pad="C1"/>
<connect gate="1" pin="C2" pad="C2"/>
<connect gate="1" pin="C3" pad="C3"/>
<connect gate="1" pin="D" pad="D"/>
<connect gate="1" pin="D1" pad="D1"/>
<connect gate="1" pin="D2" pad="D2"/>
<connect gate="1" pin="D3" pad="D3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITT-RTBCD" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
<gates>
<gate name="1" symbol="DS-BCD"/>
</gates>
<devices>
<device name="" package="ITT-RTBCD">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="1/" pad="1/"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="2/" pad="2/"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="4/" pad="4/"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="8/" pad="8/"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="C@" pad="C@"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITT-RT112" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
<gates>
<gate name="1" symbol="DS-112"/>
</gates>
<devices>
<device name="" package="ITT-RT112">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="C@" pad="C@"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITT-RT206" prefix="S" uservalue="yes">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon</description>
<gates>
<gate name="1" symbol="DS-206"/>
</gates>
<devices>
<device name="" package="ITT-RT206">
<connects>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="21" pad="21"/>
<connect gate="1" pin="22" pad="22"/>
<connect gate="1" pin="31" pad="31"/>
<connect gate="1" pin="32" pad="32"/>
<connect gate="1" pin="41" pad="41"/>
<connect gate="1" pin="42" pad="42"/>
<connect gate="1" pin="51" pad="51"/>
<connect gate="1" pin="52" pad="52"/>
<connect gate="1" pin="61" pad="61"/>
<connect gate="1" pin="62" pad="62"/>
<connect gate="1" pin="S1" pad="C1"/>
<connect gate="1" pin="S2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9070-1W" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
 Marquardt</description>
<gates>
<gate name="2" symbol="KS-UB"/>
</gates>
<devices>
<device name="" package="9070-1W">
<connects>
<connect gate="2" pin="B" pad="B"/>
<connect gate="2" pin="B1" pad="B1"/>
<connect gate="2" pin="O" pad="1"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9070-2W" prefix="S" uservalue="yes">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
 Marquardt</description>
<gates>
<gate name="B" symbol="U2"/>
<gate name="1" symbol="KS-UB-"/>
</gates>
<devices>
<device name="" package="9070-2W">
<connects>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="B1" pad="B1"/>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="B" pin="P" pad="5"/>
<connect gate="B" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REKN" prefix="S" uservalue="yes">
<description>&lt;b&gt;PUSH SWITCH&lt;/b&gt;&lt;p&gt;
ITT-Cannon-Cannon</description>
<gates>
<gate name="G$1" symbol="NORMOPEN"/>
</gates>
<devices>
<device name="" package="REKN">
<connects>
<connect gate="G$1" pin="0@A" pad="0A"/>
<connect gate="G$1" pin="0@B" pad="0B"/>
<connect gate="G$1" pin="1@A" pad="1A"/>
<connect gate="G$1" pin="1@B" pad="1B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MARQ6425" prefix="S" uservalue="yes">
<description>&lt;b&gt;DIL SWITCH&lt;/b&gt;&lt;p&gt;
with LED, Marquardt</description>
<gates>
<gate name="LED" symbol="LED"/>
<gate name="." symbol="DS"/>
</gates>
<devices>
<device name="" package="MARQ6425">
<connects>
<connect gate="." pin="P" pad="1"/>
<connect gate="." pin="S" pad="2"/>
<connect gate="LED" pin="A" pad="A"/>
<connect gate="LED" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RDT1034" prefix="S">
<description>&lt;b&gt;PUSH SWITCH&lt;/b&gt;&lt;p&gt;
www.radiohm.com</description>
<gates>
<gate name="G$1" symbol="NORMOPEN2-1"/>
</gates>
<devices>
<device name="" package="RDT1034">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SKHMP*E010" prefix="S">
<description>&lt;b&gt;6.2 X 6.5mm TACT Switch (SMD)&lt;/b&gt;&lt;p&gt;
Source: http://www3.alps.co.jp/WebObjects/catalog.woa/PDF/E/Switch/Tact/SKHM/SKHM.PDF</description>
<gates>
<gate name="G$1" symbol="NORMOPEN_SHIELD"/>
</gates>
<devices>
<device name="" package="SKHMPXE010">
<connects>
<connect gate="G$1" pin="1.1" pad="1"/>
<connect gate="G$1" pin="1.2" pad="2"/>
<connect gate="G$1" pin="2.1" pad="3"/>
<connect gate="G$1" pin="2.2" pad="4"/>
<connect gate="G$1" pin="SH" pad="5"/>
</connects>
<technologies>
<technology name="S"/>
<technology name="U"/>
<technology name="W"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSRM1" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A112"/>
</gates>
<devices>
<device name="C6200" package="SSRM1C6200">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C5400" package="SRRM1C5400">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM254700" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
2 Pole 5 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-205"/>
</gates>
<devices>
<device name="" package="SRRM254700">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="8"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="9"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="10"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="11"/>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="C2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM2" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
2 Pole 6 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A206"/>
</gates>
<devices>
<device name="62400" package="SRRM262400">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="C" pad="14"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="C4" pad="10"/>
<connect gate="G$1" pin="C5" pad="11"/>
<connect gate="G$1" pin="C6" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="63700" package="SRRM263700">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="C" pad="14"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="C4" pad="10"/>
<connect gate="G$1" pin="C5" pad="11"/>
<connect gate="G$1" pin="C6" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="64300" package="SRRM264300">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="C" pad="14"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="C4" pad="10"/>
<connect gate="G$1" pin="C5" pad="11"/>
<connect gate="G$1" pin="C6" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM342800" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
3 Pole 4 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A304"/>
</gates>
<devices>
<device name="" package="SRRM342800">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="8"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="C" pad="15"/>
<connect gate="G$1" pin="C1" pad="11"/>
<connect gate="G$1" pin="C2" pad="12"/>
<connect gate="G$1" pin="C3" pad="1"/>
<connect gate="G$1" pin="C4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM433700" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
4 Pole 3 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A403"/>
</gates>
<devices>
<device name="" package="SRRM433700">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="6"/>
<connect gate="G$1" pin="C" pad="15"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="D" pad="16"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM1C7800" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
1 Pole 12 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="SSRM-4-1"/>
</gates>
<devices>
<device name="" package="SRRM-4">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="6"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="D" pad="15"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRRM265900" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
2 Pole 6 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="SSRM-4-2"/>
</gates>
<devices>
<device name="" package="SRRM265900">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="6"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="D" pad="15"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-1X6" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-106"/>
</gates>
<devices>
<device name="" package="ELMA-01-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="11"/>
<connect gate="G$1" pin="S" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-1X10MA" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-110"/>
</gates>
<devices>
<device name="" package="ELMA-01-1X10MA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-1X10OA" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-110"/>
</gates>
<devices>
<device name="" package="ELMA-01-1X10OA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-1X11" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-111"/>
</gates>
<devices>
<device name="" package="ELMA-01-1X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-1X12" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A112"/>
</gates>
<devices>
<device name="" package="ELMA-01-1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-2X3" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A203"/>
</gates>
<devices>
<device name="" package="ELMA-01-2X3">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="1A"/>
<connect gate="G$1" pin="A2" pad="2A"/>
<connect gate="G$1" pin="A3" pad="3A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B1" pad="1B"/>
<connect gate="G$1" pin="B2" pad="2B"/>
<connect gate="G$1" pin="B3" pad="3B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-2X6" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-206"/>
</gates>
<devices>
<device name="" package="ELMA-01-2X6">
<connects>
<connect gate="G$1" pin="11" pad="1A"/>
<connect gate="G$1" pin="12" pad="1B"/>
<connect gate="G$1" pin="21" pad="2A"/>
<connect gate="G$1" pin="22" pad="2B"/>
<connect gate="G$1" pin="31" pad="3A"/>
<connect gate="G$1" pin="32" pad="3B"/>
<connect gate="G$1" pin="41" pad="4A"/>
<connect gate="G$1" pin="42" pad="4B"/>
<connect gate="G$1" pin="51" pad="5A"/>
<connect gate="G$1" pin="52" pad="5B"/>
<connect gate="G$1" pin="61" pad="6A"/>
<connect gate="G$1" pin="62" pad="6B"/>
<connect gate="G$1" pin="S1" pad="A"/>
<connect gate="G$1" pin="S2" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-4X2" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A402"/>
</gates>
<devices>
<device name="" package="ELMA-01-4X2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="1A"/>
<connect gate="G$1" pin="A2" pad="2A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B1" pad="1B"/>
<connect gate="G$1" pin="B2" pad="2B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="C1" pad="1C"/>
<connect gate="G$1" pin="C2" pad="2C"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="D1" pad="1D"/>
<connect gate="G$1" pin="D2" pad="2D"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELMA-01-4X3" prefix="S">
<description>&lt;b&gt;Rotary Switches Type 01&lt;/b&gt;&lt;p&gt;
Source: http://www.elma.com/files/products/rotary_components/pdfs/rotary_switches_type_01_002.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A403"/>
</gates>
<devices>
<device name="" package="ELMA-01-4X3">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="1A"/>
<connect gate="G$1" pin="A2" pad="2A"/>
<connect gate="G$1" pin="A3" pad="3A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B1" pad="1B"/>
<connect gate="G$1" pin="B2" pad="2B"/>
<connect gate="G$1" pin="B3" pad="3B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="C1" pad="1C"/>
<connect gate="G$1" pin="C2" pad="2C"/>
<connect gate="G$1" pin="C3" pad="3C"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="D1" pad="1D"/>
<connect gate="G$1" pin="D2" pad="2D"/>
<connect gate="G$1" pin="D3" pad="3D"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-30-A1" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A112"/>
</gates>
<devices>
<device name="-30A1" package="71BT-30-A1">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="10" pad="A10"/>
<connect gate="G$1" pin="11" pad="A11"/>
<connect gate="G$1" pin="12" pad="A12"/>
<connect gate="G$1" pin="2" pad="A2"/>
<connect gate="G$1" pin="3" pad="A3"/>
<connect gate="G$1" pin="4" pad="A4"/>
<connect gate="G$1" pin="5" pad="A5"/>
<connect gate="G$1" pin="6" pad="A6"/>
<connect gate="G$1" pin="7" pad="A7"/>
<connect gate="G$1" pin="8" pad="A8"/>
<connect gate="G$1" pin="9" pad="A9"/>
<connect gate="G$1" pin="A" pad="A-C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-30-AB1" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-A112"/>
<gate name="B" symbol="DS-A112"/>
</gates>
<devices>
<device name="" package="71BT-30-AB1">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="10" pad="A10"/>
<connect gate="A" pin="11" pad="A11"/>
<connect gate="A" pin="12" pad="A12"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="9" pad="A9"/>
<connect gate="A" pin="A" pad="A-C1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="10" pad="B10"/>
<connect gate="B" pin="11" pad="B11"/>
<connect gate="B" pin="12" pad="B12"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="9" pad="B9"/>
<connect gate="B" pin="A" pad="B-C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-30-A2" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-206"/>
</gates>
<devices>
<device name="" package="71BT-30-A2">
<connects>
<connect gate="A" pin="11" pad="A1"/>
<connect gate="A" pin="12" pad="A7"/>
<connect gate="A" pin="21" pad="A2"/>
<connect gate="A" pin="22" pad="A8"/>
<connect gate="A" pin="31" pad="A3"/>
<connect gate="A" pin="32" pad="A9"/>
<connect gate="A" pin="41" pad="A4"/>
<connect gate="A" pin="42" pad="A10"/>
<connect gate="A" pin="51" pad="A5"/>
<connect gate="A" pin="52" pad="A11"/>
<connect gate="A" pin="61" pad="A6"/>
<connect gate="A" pin="62" pad="A12"/>
<connect gate="A" pin="S1" pad="A-C1"/>
<connect gate="A" pin="S2" pad="A-C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-30-AB2" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-206"/>
<gate name="B" symbol="DS-206"/>
</gates>
<devices>
<device name="" package="71BT-30-AB2">
<connects>
<connect gate="A" pin="11" pad="A1"/>
<connect gate="A" pin="12" pad="A7"/>
<connect gate="A" pin="21" pad="A2"/>
<connect gate="A" pin="22" pad="A8"/>
<connect gate="A" pin="31" pad="A3"/>
<connect gate="A" pin="32" pad="A9"/>
<connect gate="A" pin="41" pad="A4"/>
<connect gate="A" pin="42" pad="A10"/>
<connect gate="A" pin="51" pad="A5"/>
<connect gate="A" pin="52" pad="A11"/>
<connect gate="A" pin="61" pad="A6"/>
<connect gate="A" pin="62" pad="A12"/>
<connect gate="A" pin="S1" pad="A-C1"/>
<connect gate="A" pin="S2" pad="A-C2"/>
<connect gate="B" pin="11" pad="B1"/>
<connect gate="B" pin="12" pad="B7"/>
<connect gate="B" pin="21" pad="B2"/>
<connect gate="B" pin="22" pad="B8"/>
<connect gate="B" pin="31" pad="B3"/>
<connect gate="B" pin="32" pad="B9"/>
<connect gate="B" pin="41" pad="B4"/>
<connect gate="B" pin="42" pad="B10"/>
<connect gate="B" pin="51" pad="B5"/>
<connect gate="B" pin="52" pad="B11"/>
<connect gate="B" pin="61" pad="B6"/>
<connect gate="B" pin="62" pad="B12"/>
<connect gate="B" pin="S1" pad="B-C1"/>
<connect gate="B" pin="S2" pad="B-C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-36-A1" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-110"/>
</gates>
<devices>
<device name="" package="71BT-36-A1">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="10" pad="A10"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="9" pad="A9"/>
<connect gate="A" pin="S" pad="A-C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-36-A2" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-205"/>
</gates>
<devices>
<device name="" package="71BT-36-A2">
<connects>
<connect gate="A" pin="11" pad="A1"/>
<connect gate="A" pin="12" pad="A6"/>
<connect gate="A" pin="21" pad="A2"/>
<connect gate="A" pin="22" pad="A7"/>
<connect gate="A" pin="31" pad="A3"/>
<connect gate="A" pin="32" pad="A8"/>
<connect gate="A" pin="41" pad="A4"/>
<connect gate="A" pin="42" pad="A9"/>
<connect gate="A" pin="51" pad="A5"/>
<connect gate="A" pin="52" pad="A10"/>
<connect gate="A" pin="C1" pad="A-C1"/>
<connect gate="A" pin="C2" pad="A-C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-36-AB1" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-110"/>
<gate name="B" symbol="DS-110"/>
</gates>
<devices>
<device name="" package="71BT-36-AB1">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="10" pad="A10"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="9" pad="A9"/>
<connect gate="A" pin="S" pad="A-C1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="10" pad="B10"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="9" pad="B9"/>
<connect gate="B" pin="S" pad="B-C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="71BT-36-AB2" prefix="S">
<description>&lt;b&gt;Multi-Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-31-44.pdf</description>
<gates>
<gate name="A" symbol="DS-205"/>
<gate name="B" symbol="DS-205"/>
</gates>
<devices>
<device name="" package="71BT-36-AB2">
<connects>
<connect gate="A" pin="11" pad="A1"/>
<connect gate="A" pin="12" pad="A6"/>
<connect gate="A" pin="21" pad="A2"/>
<connect gate="A" pin="22" pad="A7"/>
<connect gate="A" pin="31" pad="A3"/>
<connect gate="A" pin="32" pad="A8"/>
<connect gate="A" pin="41" pad="A4"/>
<connect gate="A" pin="42" pad="A9"/>
<connect gate="A" pin="51" pad="A5"/>
<connect gate="A" pin="52" pad="A10"/>
<connect gate="A" pin="C1" pad="A-C1"/>
<connect gate="A" pin="C2" pad="A-C2"/>
<connect gate="B" pin="11" pad="B1"/>
<connect gate="B" pin="12" pad="B6"/>
<connect gate="B" pin="21" pad="B2"/>
<connect gate="B" pin="22" pad="B7"/>
<connect gate="B" pin="31" pad="B3"/>
<connect gate="B" pin="32" pad="B8"/>
<connect gate="B" pin="41" pad="B4"/>
<connect gate="B" pin="42" pad="B9"/>
<connect gate="B" pin="51" pad="B5"/>
<connect gate="B" pin="52" pad="B10"/>
<connect gate="B" pin="C1" pad="B-C1"/>
<connect gate="B" pin="C2" pad="B-C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75?36-1-10" prefix="S">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
<gates>
<gate name="G$1" symbol="DS-110"/>
</gates>
<devices>
<device name="AF" package="75AF36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AP" package="75AP36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BF" package="75BF36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BP" package="75BP36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CF" package="75CF36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="75CP36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-1POLE22,5" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches one pole 22.5°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-116"/>
</gates>
<devices>
<device name="" package="50-1POLE22,5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="C" pad="C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-1POLE30" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches one pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A112"/>
</gates>
<devices>
<device name="" package="50-1POLE30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-2POLE22,5" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches two pole 22.5°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-208"/>
</gates>
<devices>
<device name="" package="50-2POLE22,5">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="9"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="10"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="11"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="12"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="13"/>
<connect gate="G$1" pin="61" pad="6"/>
<connect gate="G$1" pin="62" pad="14"/>
<connect gate="G$1" pin="71" pad="7"/>
<connect gate="G$1" pin="72" pad="15"/>
<connect gate="G$1" pin="81" pad="8"/>
<connect gate="G$1" pin="82" pad="16"/>
<connect gate="G$1" pin="S1" pad="C1"/>
<connect gate="G$1" pin="S2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-2POLE30" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches two pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-206"/>
</gates>
<devices>
<device name="" package="50-2POLE30">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="8"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="9"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="10"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="11"/>
<connect gate="G$1" pin="61" pad="6"/>
<connect gate="G$1" pin="62" pad="12"/>
<connect gate="G$1" pin="S1" pad="C1"/>
<connect gate="G$1" pin="S2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-3POLE30" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches three pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A304"/>
</gates>
<devices>
<device name="" package="50-3POLE30">
<connects>
<connect gate="G$1" pin="A" pad="C1"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="B" pad="C2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="B3" pad="7"/>
<connect gate="G$1" pin="B4" pad="8"/>
<connect gate="G$1" pin="C" pad="C3"/>
<connect gate="G$1" pin="C1" pad="9"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="11"/>
<connect gate="G$1" pin="C4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-4POLE30" prefix="S">
<description>&lt;b&gt;SERIES 50&lt;/b&gt; Single-Deck Rotary Switches four pole 30°&lt;p&gt;
Source: www.grayhill.com .. J-15-21.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A403"/>
</gates>
<devices>
<device name="" package="50-4POLE30">
<connects>
<connect gate="G$1" pin="A" pad="C1"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="B" pad="C2"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="6"/>
<connect gate="G$1" pin="C" pad="C3"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="D" pad="C4"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24-1POLE36" prefix="S">
<description>&lt;b&gt;SERIES 24&lt;/b&gt; Rotary Switches one pole 36°&lt;p&gt;
Source: www.grayhill.com .. J-28.pdf</description>
<gates>
<gate name="G$1" symbol="DS-110"/>
</gates>
<devices>
<device name="" package="24-1POLE36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75?36-2" prefix="S">
<description>&lt;b&gt;Single Deck Rotary Switches&lt;/b&gt;&lt;p&gt;
Source: www.grayhill.com .. J-13-14.pdf</description>
<gates>
<gate name="G$1" symbol="DS-205"/>
</gates>
<devices>
<device name="AF" package="75AF36-2">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="6"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="7"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="8"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="9"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="10"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AP" package="75AP36-2">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="6"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="7"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="8"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="9"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="10"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BF" package="75BF36-2">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="6"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="7"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="8"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="9"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="10"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BP" package="75BP36-2">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="6"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="7"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="8"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="9"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="10"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CF" package="75CF36-2">
<connects>
<connect gate="G$1" pin="11" pad="1"/>
<connect gate="G$1" pin="12" pad="6"/>
<connect gate="G$1" pin="21" pad="2"/>
<connect gate="G$1" pin="22" pad="7"/>
<connect gate="G$1" pin="31" pad="3"/>
<connect gate="G$1" pin="32" pad="8"/>
<connect gate="G$1" pin="41" pad="4"/>
<connect gate="G$1" pin="42" pad="9"/>
<connect gate="G$1" pin="51" pad="5"/>
<connect gate="G$1" pin="52" pad="10"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CK10" prefix="S">
<description>&lt;b&gt;ROTARY SWITCH&lt;/b&gt;&lt;p&gt;
C&amp;K</description>
<gates>
<gate name="G$1" symbol="DS-A403"/>
</gates>
<devices>
<device name="" package="CK10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="6"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="C1" pad="7"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="9"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL36PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="U"/>
</gates>
<devices>
<device name="" package="TL3XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL39PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON"/>
</gates>
<devices>
<device name="" package="TL3XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL37PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL38PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL32PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM"/>
</gates>
<devices>
<device name="" package="TL3XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL42PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL46PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="U_2"/>
</gates>
<devices>
<device name="" package="TL4XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL47PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL48PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL49PO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON_2"/>
</gates>
<devices>
<device name="" package="TL4XPO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL36YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="U"/>
</gates>
<devices>
<device name="" package="TL3XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL39YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON"/>
</gates>
<devices>
<device name="" package="TL3XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL37YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL38YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL32YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM"/>
</gates>
<devices>
<device name="" package="TL3XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL42YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL46YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="U_2"/>
</gates>
<devices>
<device name="" package="TL4XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL47YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL48YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL49YO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON_2"/>
</gates>
<devices>
<device name="" package="TL4XYO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL36WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="U"/>
</gates>
<devices>
<device name="" package="TL3XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL39WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON"/>
</gates>
<devices>
<device name="" package="TL3XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL37WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL38WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM"/>
</gates>
<devices>
<device name="" package="TL3XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL32WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM"/>
</gates>
<devices>
<device name="" package="TL3XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL42WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL46WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON - ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="U_2"/>
</gates>
<devices>
<device name="" package="TL4XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL47WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; MOM OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="MOM-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL48WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF MOM&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-MOM_2"/>
</gates>
<devices>
<device name="" package="TL4XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL49WO" prefix="S">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt; ON OFF ON&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36WO.pdf</description>
<gates>
<gate name="BEF1" symbol="ON-OFF-ON_2"/>
</gates>
<devices>
<device name="" package="TL4XWO">
<connects>
<connect gate="BEF1" pin="O" pad="1"/>
<connect gate="BEF1" pin="O1" pad="4"/>
<connect gate="BEF1" pin="P" pad="2"/>
<connect gate="BEF1" pin="P1" pad="5"/>
<connect gate="BEF1" pin="S" pad="3"/>
<connect gate="BEF1" pin="S1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="55?" prefix="S">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt;&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
<gates>
<gate name="G$1" symbol="NO-NC-2"/>
</gates>
<devices>
<device name="01" package="5501">
<connects>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="11" package="5511">
<connects>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="55?-1LED" prefix="S">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt; 1 LED&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
<gates>
<gate name="-1" symbol="NO-NC-2"/>
<gate name="-LED" symbol="LED"/>
</gates>
<devices>
<device name="01" package="5501-1LED">
<connects>
<connect gate="-1" pin="1A" pad="1A"/>
<connect gate="-1" pin="1B" pad="1B"/>
<connect gate="-1" pin="NC" pad="NC"/>
<connect gate="-1" pin="NO" pad="NO"/>
<connect gate="-LED" pin="A" pad="+"/>
<connect gate="-LED" pin="K" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="11" package="5511-1LED">
<connects>
<connect gate="-1" pin="1A" pad="1A"/>
<connect gate="-1" pin="1B" pad="1B"/>
<connect gate="-1" pin="NC" pad="NC"/>
<connect gate="-1" pin="NO" pad="NO"/>
<connect gate="-LED" pin="A" pad="+G"/>
<connect gate="-LED" pin="K" pad="-G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="55?-2LED" prefix="S">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt; 2 LED&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
<gates>
<gate name="-1" symbol="NO-NC-2"/>
<gate name="-LED1" symbol="LED"/>
<gate name="-LED2" symbol="LED"/>
</gates>
<devices>
<device name="01" package="5501-2LED">
<connects>
<connect gate="-1" pin="1A" pad="1A"/>
<connect gate="-1" pin="1B" pad="1B"/>
<connect gate="-1" pin="NC" pad="NC"/>
<connect gate="-1" pin="NO" pad="NO"/>
<connect gate="-LED1" pin="A" pad="+R"/>
<connect gate="-LED1" pin="K" pad="-R"/>
<connect gate="-LED2" pin="A" pad="+G"/>
<connect gate="-LED2" pin="K" pad="-G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="11" package="5511-2LED">
<connects>
<connect gate="-1" pin="1A" pad="1A"/>
<connect gate="-1" pin="1B" pad="1B"/>
<connect gate="-1" pin="NC" pad="NC"/>
<connect gate="-1" pin="NO" pad="NO"/>
<connect gate="-LED1" pin="A" pad="+Y"/>
<connect gate="-LED1" pin="K" pad="-Y"/>
<connect gate="-LED2" pin="A" pad="+R"/>
<connect gate="-LED2" pin="K" pad="-R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2P2T" prefix="S">
<description>&lt;b&gt;SLIDE SWITCH 2P2T&lt;/b&gt; Part No. SS-22F05-G(A)4&lt;p&gt;
Source: CANAL ELECTRONIC CO., LTD .. switsch.pdf</description>
<gates>
<gate name="G$1" symbol="2P2T"/>
</gates>
<devices>
<device name="" package="2P2T">
<connects>
<connect gate="G$1" pin="1.1" pad="1.1"/>
<connect gate="G$1" pin="1.2" pad="1.2"/>
<connect gate="G$1" pin="2.1" pad="2.1"/>
<connect gate="G$1" pin="2.2" pad="2.2"/>
<connect gate="G$1" pin="3.1" pad="3.1"/>
<connect gate="G$1" pin="3.2" pad="3.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3PDT" prefix="S">
<description>&lt;b&gt;3PDT 9 pin footswitch&lt;/b&gt; SF17020F-0302-21R-L&lt;p&gt;
Source: 3PDT.jpg</description>
<gates>
<gate name="G$1" symbol="U_3L"/>
</gates>
<devices>
<device name="" package="3PDT">
<connects>
<connect gate="G$1" pin="O1" pad="1"/>
<connect gate="G$1" pin="O2" pad="4"/>
<connect gate="G$1" pin="O3" pad="7"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P2" pad="5"/>
<connect gate="G$1" pin="P3" pad="8"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="6"/>
<connect gate="G$1" pin="S3" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
